#

12.1 Cassette Deck Section

TOP PREVIOUS NEXT

- Measurement Condition

  - Make sure head, capstan and press roller are clean.

  - Judgeable room temperature 20 ± 5 °C (68 ± 9°F)

- Measuring instrument

  - EVM (Electronic Volmeter)

  - Digital quency counter

- Test Tape

  - Tape speed gain adjustment (3 kHz, -10 dB); QZZCWAT

12.1.1 Tape Speed Adjustment (Deck 1/2)

12.1.2 Bias and Erase Voltage Check

12.1.3 Bias Frequency Adjustment (Deck 1/2)

TOP PREVIOUS NEXT