<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-AK200</Model>
<System>ORDER NO. MD0112227C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1202010000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=2 month=Oct year=2002>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-AK200</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>12.2.1 AM-IF Alignment</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1202000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1203000000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para><emphasis>AM-IF ALIGNMENT</emphasis>
</Para>
</item>
</randlist>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="6" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="1.060in">
<colspec colnum="2" colname="2" colwidth="1.034in">
<colspec colnum="3" colname="3" colwidth="1.210in">
<colspec colnum="4" colname="4" colwidth="1.296in">
<colspec colnum="5" colname="5" colwidth="1.513in">
<colspec colnum="6" colname="6" colwidth="1.090in">
<thead><row rowsep="1"><entry namest="1" nameend="2" align="center"><Para>SIGNAL GENERATOR OR SWEEP GENERATOR</Para>
</entry>
<entry colname="3" morerows="1" align="center"><Para>RADIO DIAL SETTING</Para>
</entry>
<entry colname="4" morerows="1" align="center"><Para>INDICATOR (ELECTRONIC VOLTMETER OSCILLOSCOPE)</Para>
</entry>
<entry colname="5" morerows="1" align="center"><Para><emphasis>ADJUSTMENT(Shown in Fig.3)</emphasis>
</Para>
</entry>
<entry colname="6" morerows="1" align="center"><Para>REMARKS</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>CONNECTIONS</Para>
</entry>
<entry colname="2" align="center"><Para>FREQUENCY</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="0"><entry colname="1" align="left"><Para>Fashion a loop of several turns of wire and radiate signal into loop of receiver.</Para>
</entry>
<entry colname="2" align="left"><Para>450 kHz 30&percnt; Mod. at 40Hz.</Para>
</entry>
<entry colname="3" align="left"><Para>Point of non-interference (on&sol;about 600 kHz)</Para>
</entry>
<entry colname="4" align="left"><Para>Headphone Jack (32&ohm;) Fabricate the plug as shown in Fig. 2 and then connect the lead wires of the plug to the measuring instrument.</Para>
</entry>
<entry colname="5" align="left"><Para>Z102 (AM IFT)</Para>
</entry>
<entry colname="6" align="left"><Para>Adjust for maximum output.</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para></Para>
<Para><randlist prefix=unorder><item><Para><emphasis>AM-RF ALIGNMENT</emphasis>
</Para>
</item>
</randlist>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="6" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.966in">
<colspec colnum="2" colname="2" colwidth="0.988in">
<colspec colnum="3" colname="3" colwidth="1.226in">
<colspec colnum="4" colname="4" colwidth="1.401in">
<colspec colnum="5" colname="5" colwidth="1.551in">
<colspec colnum="6" colname="6" colwidth="1.069in">
<thead><row rowsep="1"><entry namest="1" nameend="2" align="center"><Para>SIGNAL GENERATOR OR SWEEP GENERATOR</Para>
</entry>
<entry colname="3" morerows="1" align="center"><Para>RADIO DIAL SETTING</Para>
</entry>
<entry colname="4" morerows="1" align="center"><Para><emphasis>INDICATOR (ELECTRONIC VOLTMETER OSCILLOSCOPE)</emphasis>
</Para>
</entry>
<entry colname="5" morerows="1" align="center"><Para><emphasis>ADJUSTMENT(Shown in Fig.1)</emphasis>
</Para>
</entry>
<entry colname="6" morerows="1" align="center"><Para>REMARKS</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>CONNECTIONS</Para>
</entry>
<entry colname="2" align="center"><Para>FREQUENCY</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="left"><Para>Fashion a loop of several turns of wire and radiate signal into loop of receiver.</Para>
</entry>
<entry colname="2" align="left"><Para>520 kHz </Para>
</entry>
<entry colname="3" align="left"><Para>Tuning capacitor fully closed.</Para>
</entry>
<entry colname="4" align="left"><Para>Headphone Jack (32&ohm;) Fabricate the plug as shown in Fig. 2 and then connect the lead wires of the plug to the measuring instrument.</Para>
</entry>
<entry colname="5" align="left"><Para>Z101 (AM OSC Coil)</Para>
</entry>
<entry colname="6" align="left"><Para>Adjust for maximum output.</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="left"><Para>Fashion a loop of several turns of wire and radiate signal into loop of receiver.</Para>
</entry>
<entry colname="2" align="left"><Para>600 kHz </Para>
</entry>
<entry colname="3" align="justify"><Para>Tuning capacitor fully open.</Para>
</entry>
<entry colname="4" align="left"><Para>Headphone Jack (32&ohm;) Fabricate the plug as shown in Fig. 2 and then connect the lead wires of the plug to the measuring instrument.</Para>
</entry>
<entry colname="5" align="justify"><Para>Z101 (AM ANT Coil)</Para>
</entry>
<entry colname="6" align="left"><Para>Adjust for maximum output.</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1202000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1203000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
