#

Service Manual

TOP NEXT

ORDER NO. MD0112227C1

A6

CD Stereo System

- SA-AK200

Colour

(S)... Silver Type

Area

(P)... U.S.A.

(PC)... Canada

TAPE SECTION :

SG-2W MECHANISM SERIES

CD SECTION :

RAE0152Z-3 TRAVERSE DECK SERIES

Specifications
AMPLIFIER SECTION |
Power output |
10% Total harmonic distortion
3 kHz - 16 kHz, both channels driven
(HIGH) | 30 W per channel (6Ω)
60 Hz - 3 kHz, both channels driven
(LOW) | 30 W per channel (6Ω)
Total Bi-Amp power | 60 W per channel
Power output |
10% Total harmonic distortion
10 kHz, both channels driven
(HIGH) | 37 W per channel (6Ω)
1 kHz, both channels driven
(LOW) | 38 W per channel (6Ω)
Total Bi-Amp power | 75 W per channel
Input sensitivity |
AUX | 250 mV
Input Impedance |
AUX | 13.3 kΩ
FM TUNER SECTION |
Frequency range | 87.9 - 107.9 MHz (200 kHz steps)
| 87.5 - 108.0 MHz (100 kHz steps)
Sensitivity | 2.5μV (IHF)
S/N 26 dB | 2.2μV
Antenna terminal(s) | 75Ω (unbalanced)
AM TUNER SECTION |
Frequency range | 520 - 1710 kHz (10 kHz steps)
Sensitivity |
S/N 20 dB (at 1000 kHz) | 560μV/m
CASSETTE DECK SECTION |
Track system | 4 track, 2 channel
Heads |
Record/playback | Solid permalloy head
Erasure | Double gap ferrite head
Motor | DC servo motor
Recording system | AC bias 100 kHz
Erasing system | AC erase 100 kHz
Tape speed | 4.8 cm/s
Frequency response (+3 dB, -6 dB at DECK OUT)
NORMAL (TYPE I) | 35 Hz - 14 kHz
S/N | 50 dB (A weighted)
Wow and flutter | 0.18% (WRMS)
Fast forward and rewind time | Approx. 120 seconds with
| C-60 cassette tape
CD SECTION |
Sampling frequency | 44.1 kHz
Decoding | 16 bit linear
Beam source/wave length | Semiconductor laser/780 nm
Number of channels | Stereo
Frequency response | 20 Hz - 20 kHz (+1, -2 dB)
Wow and flutter | Below measurable limit
Digital filter | 8 fs
D/A converter | MASH (1 bit DAC)
GENERAL |
Power supply | AC 120 V, 60Hz
Power consumption | 150 W
Power consumption in standby mode
| 0.34 W
Dimensions (W x H x D) | 250 x 315 x 345 mm
| (9 27/32” x 12 13/32” x 13 19/32”)
Mass | 6.9 kg (15.2 lb)
SYSTEM |
SC-AK200(P) | Music Center: SA-AK200(P)
| Speaker: SB-AK200(P)
SC-AK200(PC) | Music Center: SA-AK200(PC)
| Speaker: SB-AK200(P)
Notes: Specifications are subject to change without notice. Mass and dimensions are aproximate. Total harmonic distortion is measured by the digital spectrum analyzer. The labels“HIGH” and“LOW” on the rear of the speakers refer to High frequency and Low frequency.

© 2001 Matsushita Electronics (S) Pte. Ltd. All rights reserved. Unauthorized copying and distribution is a violation of law.

TOP NEXT