#

10.2 Error detection for CD/Changer block

TOP PREVIOUS NEXT

No. | Error | ErrorDisplay | Problem condition
1 | REST SW detection error | F15 | CD does not function.This error occurs when the Optical Pick Up REST SW (S701) is not detected within the specified time (about 8 seconds)
2 | CD tray opens automatically | F16 | CLAMP switch (S4) NG (Check & Replace)
3 | Does not startup when [PLAY]button is pressed | F17 | BOTTOM switch (S5) NG (Check & Replace)
4 | Transmission error between CDservo LSI and micon | F26 | CD does not function.This error occurs when the POWER is ON for the CD block and an error is detected after the transmission has started.
5 | Startup fails even when youinsert CD or the selected disc tray does not open | F27 | Tray 1 detect switch or Tray 2 detect switch NG (Check & Replace)
6 | Cannot insert CD | F28 | Tray 1 detect switch NG (Check & Replace)
7 | Cannot eject CD | F29 | Check if disc is stuck. Tray 2 detect switch NG (Confirm & Replace)
8 | The CD tray closes | H15 | CD disc tray detect switch NG (S3) (Check & Replace)

TOP PREVIOUS NEXT