#

10.1 Error detection for Cassette Mechanism block

TOP PREVIOUS NEXT

No. | Error | ErrorDisplay | Problem condition
1 | MODE SWdetection error | H01 | Faulty operation of cassette mechanism.Faulty contact or short-circuit of mechanism mode switch (S951, S971).
2 | REC INH SWdetection error | H02 | Recording not possible.Faulty contact or short-circuit of REC INH switch (S974, S975).
3 | HALF SWdetection error | H03 | Playback cannot perform.Faulty contact or short-circuit of HALF siwtch (S952, S972).
4 | Reel Pulsedetection error | F01 | The tape advances slightly and then stops.Faulty reel pulse, faulty hole detect IC (IC951, IC971).
5 | TPS abnormal | F02 | Cassette deck will not perform TPS function.Faulty playback EQ/recording amplifier IC (IC101).

TOP PREVIOUS NEXT