<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-AK200</Model>
<System>ORDER NO. MD0112227C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0801010000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=2 month=Oct year=2002>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-AK200</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>8.1.1 Checking of the Main, Panel, Transformer and Deck P.C.B.</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0801000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0802000000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>Step 1</emphasis>
 Remove 3 screws each side and 5 screws at rear panel.</Para>
<Figure><graphic boardno="graphic13" reprowid="68.411mm" reprodep="85.514mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
 Remove the Top Cabinet.</Para>
<Figure><graphic boardno="graphic14" reprowid="67.056mm" reprodep="99.229mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
 Push the lever in the direction of the arrow.</Para>
<Figure><graphic boardno="graphic15" reprowid="62.484mm" reprodep="91.779mm" location="internal"></Figure>
<Figure><graphic boardno="graphic16" reprowid="57.912mm" reprodep="39.285mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Pull out the CD tray as shown and remove the CD lid.               Push back the CD tray after the CD lid has been              removed. </Para>
<Figure><graphic boardno="graphic17" reprowid="68.749mm" reprodep="96.859mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
 Release the 2 catches, disconnect CN310 and remove the CD changer base together with the CD changer.</Para>
<Figure><graphic boardno="graphic18" reprowid="65.193mm" reprodep="79.926mm" location="internal"></Figure>
<Para><emphasis>Step 6 </emphasis>
Remove 8 screws.</Para>
<Para></Para>
<Para><randlist prefix=unorder><item><Para><emphasis>Checking for Main, Panel , Transformer and Deck P.C.B</emphasis>
</Para>
<Figure><graphic boardno="graphic19" reprowid="61.637mm" reprodep="79.417mm" location="internal"></Figure>
</item>
</randlist>
</Para>
<Para></Para>
<Para><randlist prefix=unorder><item><Para><emphasis>Checking for Power P.C.B.</emphasis>
</Para>
<Para><emphasis>Step  7 and 8 </emphasis>
Remove 2 screws each side.</Para>
<Figure><graphic boardno="graphic20" reprowid="64.347mm" reprodep="63.839mm" location="internal"></Figure>
<Figure><graphic boardno="graphic21" reprowid="63.839mm" reprodep="57.573mm" location="internal"></Figure>
</item>
</randlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0801000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0802000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
