#

9.3 Cassette Mechanism Test (For error code H01, H02, H03, F01, F02)

TOP PREVIOUS NEXT

1. Press “TAPE, DECK 1/2” to select Deck 2.

2. Load a cassette tape with the erasure prevention tab, remove from left side only and close the cassette holder.

3. Press “FAST FORWARD MEMORY” (Tape will be stop after 2 seconds)

4. Load a cassette tape with the erasure prevention tab, remove from right side only and close the cassette holder.

5. Press “REVERSE FM MODE/BP” (Tape will be stop after 2 seconds)

6. Load a pre-recorded tape with both side record tabs intact and close the cassette holder.

7. Press “PLAY/TUNE/TIME ADJ UP” (After TPS function, tape will stop automatically)

8. Press “REC/STOP” (Tape will not move)

9. Press “STOP/TUNE MODE” to indicate Error code.

   - If several problem exist, error code will change each time when “ /TUNE MODE” is pressed.

     (e.g. H01 → H03 → F01 .....etc.)

10. Press “TAPE, DECK 1/2” to select Deck 1.

11. Repeat step 2 to 9 to test Deck 1. (Tape Deck 1 will not check H02 because of no recording function)

TOP PREVIOUS NEXT