<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-AK200</Model>
<System>ORDER NO. MD0112227C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1404000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=2 month=Oct year=2002>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-AK200</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>14.4 IC600 (C2BBGF000335) System Microprocessor</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1403000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1500000000x
</nmlist>
</nameloc>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.831in">
<colspec colnum="2" colname="2" colwidth="0.702in">
<colspec colnum="3" colname="3" colwidth="0.400in">
<colspec colnum="4" colname="4" colwidth="1.492in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>Pin No.</Para>
</entry>
<entry colname="2" align="center"><Para><emphasis>Mark</emphasis>
</Para>
</entry>
<entry colname="3" align="center"><Para><emphasis>I&sol;O</emphasis>
</Para>
</entry>
<entry colname="4" align="center"><Para><emphasis>Function</emphasis>
</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>DECK2</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tape mecha condition input (Half2&sol;Reci_F&sol;Mode&sol;Reci_R)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY3</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 3 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY2</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 2 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY1</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 1 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>V_JOG</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Volume jog A-D detection input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_AD2</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>(Position&sol; bottom) Chngr sw A-D detection input 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_AD1</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>(Open Clamp) Chngr sw A-D detection input 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>CDRST</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD reset output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>9</Para>
</entry>
<entry colname="2" align="justify"><Para>STATUS</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD signal processor status input (INV)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>10</Para>
</entry>
<entry colname="2" align="justify"><Para>LM_L</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Level meter left</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>11</Para>
</entry>
<entry colname="2" align="justify"><Para>LM_R</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Level meter right</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>12</Para>
</entry>
<entry colname="2" align="justify"><Para>ST&sol;DO&sol;SQCK</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner if data&sol;stereo input and CD subcode clock output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>13</Para>
</entry>
<entry colname="2" align="justify"><Para>SD</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner signal detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>14</Para>
</entry>
<entry colname="2" align="justify"><Para>SUBQ</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD subcode data input (INV)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>15</Para>
</entry>
<entry colname="2" align="justify"><Para>RDS_CLK</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>RDS clock input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>16</Para>
</entry>
<entry colname="2" align="justify"><Para>RDS_DAT</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>RDS data input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>17</Para>
</entry>
<entry colname="2" align="justify"><Para>CNVSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Flash mode terminal (connect to ground)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>18</Para>
</entry>
<entry colname="2" align="justify"><Para>&sol;RESET</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>RESET input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>19</Para>
</entry>
<entry colname="2" align="justify"><Para>XCOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>32.768 kHz sub clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>20</Para>
</entry>
<entry colname="2" align="justify"><Para>XCIN</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>32.768 kHz sub clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>21</Para>
</entry>
<entry colname="2" align="justify"><Para>VSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Ground (0V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>22</Para>
</entry>
<entry colname="2" align="justify"><Para>XIN</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>4.19 MHz main clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>23</Para>
</entry>
<entry colname="2" align="justify"><Para>XOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>4.19 MHz main clock</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>24</Para>
</entry>
<entry colname="2" align="justify"><Para>VCC</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power supply (&plus;5V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>25</Para>
</entry>
<entry colname="2" align="justify"><Para>MBP1</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>MPU beat proof output 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>26</Para>
</entry>
<entry colname="2" align="justify"><Para>MBP2</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>MPU beat proof output 2</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>27</Para>
</entry>
<entry colname="2" align="justify"><Para>MCLK&sol; </Para>
<Para>PLLCK</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD command clock output&sol; tuner PLL clock output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>28</Para>
</entry>
<entry colname="2" align="justify"><Para>MDATA&sol; </Para>
<Para>PLLDA</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD command data output&sol; tuner PLL data output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>29</Para>
</entry>
<entry colname="2" align="justify"><Para>RMT</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Remote control input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>30</Para>
</entry>
<entry colname="2" align="justify"><Para>BLKCK</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD block clock input (INV)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>31</Para>
</entry>
<entry colname="2" align="justify"><Para>MLD&sol; PLLCE</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD command load output&sol; tuner PLL chip enable</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>32</Para>
</entry>
<entry colname="2" align="justify"><Para>SYNC</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>AC failure detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>33</Para>
</entry>
<entry colname="2" align="justify"><Para>DCDET</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DC detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>34</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_CCW</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer motor CCW output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>35</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_CW</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer motor CW output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>36</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_HLF</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer half drive output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>37</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_PGR</Para>
</entry>
<entry colname="3" align="justify"><Para>0</Para>
</entry>
<entry colname="4" align="justify"><Para>Changer plunger output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>38</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_SW2</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD changer SW2 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>39</Para>
</entry>
<entry colname="2" align="justify"><Para>CHG_SW1</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>CD changer SW1 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>40</Para>
</entry>
<entry colname="2" align="justify"><Para>&sol;RESTSW</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CD limit SW input for the most inner point (Active Low)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>41</Para>
</entry>
<entry colname="2" align="justify"><Para>PCONT</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Main transformer control output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>42</Para>
</entry>
<entry colname="2" align="justify"><Para>LED_3</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Backlight LED3 control</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>43</Para>
</entry>
<entry colname="2" align="justify"><Para>LED_2</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Backlight LED2 control</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>44-80</Para>
</entry>
<entry colname="2" align="justify"><Para>SEG38 - SEG2</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output (Anode drive output)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>81</Para>
</entry>
<entry colname="2" align="justify"><Para>REG8&sol;SEG1</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output. Regional&sol;Function setting use</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>82-88</Para>
</entry>
<entry colname="2" align="justify"><Para>REG7&sol;GRID7- REG1&sol;GRID1</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output (Anode drive output)For regional setting&sol; function selection use</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>89</Para>
</entry>
<entry colname="2" align="justify"><Para>VEE</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power supply (-30V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>90</Para>
</entry>
<entry colname="2" align="left"><Para>REG_IN</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Region and function setting input and eeprom chip select output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>91</Para>
</entry>
<entry colname="2" align="justify"><Para>EE_CS</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM chip select</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>92</Para>
</entry>
<entry colname="2" align="justify"><Para>SER5</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>(EE_CLK&sol;EX1_CLK)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>93</Para>
</entry>
<entry colname="2" align="justify"><Para>SER4</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>(MK_CLK_)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>94</Para>
</entry>
<entry colname="2" align="justify"><Para>SER3</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>(EE_DAT&sol;EX1_DAT)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>95</Para>
</entry>
<entry colname="2" align="justify"><Para>SER2</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>(ASP_CLK)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>96</Para>
</entry>
<entry colname="2" align="justify"><Para>SER1</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>(ASP_DATA &sol;MK_DAT)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>97</Para>
</entry>
<entry colname="2" align="justify"><Para>AVSS </Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Analog ground (0V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>98</Para>
</entry>
<entry colname="2" align="justify"><Para>VREF</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Reference for A-D</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>99</Para>
</entry>
<entry colname="2" align="justify"><Para>TPS</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>TPS&sol;Chrome1&sol;Chrome2</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>100</Para>
</entry>
<entry colname="2" align="justify"><Para>DECK1</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tape mecha condition input (Half1&sol;Mode&sol;Photo1&sol;Photo 2)</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1403000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1500000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
