#

8.1.1 Checking of the Main, Panel, Transformer and Deck P.C.B.

TOP PREVIOUS NEXT

Step 1 Remove 3 screws each side and 5 screws at rear panel.

Step 2 Remove the Top Cabinet.

Step 3 Push the lever in the direction of the arrow.

Step 4 Pull out the CD tray as shown and remove the CD lid. Push back the CD tray after the CD lid has been removed.

Step 5 Release the 2 catches, disconnect CN310 and remove the CD changer base together with the CD changer.

Step 6 Remove 8 screws.

- Checking for Main, Panel , Transformer and Deck P.C.B

- Checking for Power P.C.B.

  Step 7 and 8 Remove 2 screws each side.

TOP PREVIOUS NEXT