<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-AK200</Model>
<System>ORDER NO. MD0112227C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0803000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=2 month=Oct year=2002>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-AK200</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>8.3 Disassembly and assembly of the Traverse Unit</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0802020000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0804000000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>Step 1</emphasis>
 Push the lever from position A to B.</Para>
<Para><emphasis>Step 2</emphasis>
 Pull the stopper (black) in the direction of arrow 1 and push the lever in the direction of arrow 2.</Para>
<Para><emphasis>Step 3</emphasis>
 Push the stopper (black) down until the white lever eject out.</Para>
<Figure><graphic boardno="graphic31" reprowid="74.168mm" reprodep="87.207mm" location="internal"></Figure>
<Para><emphasis>Step 4 </emphasis>
Lift up the traverse unit and slide out the unit as shown.</Para>
<Figure><graphic boardno="graphic32" reprowid="71.120mm" reprodep="55.880mm" location="internal"></Figure>
<Para><randlist prefix=unorder><item><Para><emphasis>Replacement of Traverse Unit</emphasis>
</Para>
</item>
</randlist>
</Para>
<Para><emphasis>Step 1</emphasis>
 Place the traverse unit as shown.</Para>
<Para><emphasis>Step 2</emphasis>
 Press in the lever shaft in the direction of arrow 1 as shown and push the traverse unit into the position in the direction of arrow 2.</Para>
<Figure><graphic boardno="graphic33" reprowid="74.168mm" reprodep="65.702mm" location="internal"></Figure>
<Para><emphasis>Step 3 </emphasis>
Pull the stopper in the direction of arrow 1 and release the lever in the direction of arrow 2 as shown.</Para>
<Figure><graphic boardno="graphic34" reprowid="74.168mm" reprodep="38.608mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Pull out the tray half way and push it back fully.</Para>
<Figure><graphic boardno="graphic35" reprowid="74.168mm" reprodep="51.308mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
 Push the lever to the initial position indicated &lsquo;|---|&rsquo;.</Para>
<Figure><graphic boardno="graphic36" reprowid="74.168mm" reprodep="35.729mm" location="internal"></Figure>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0802020000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0804000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
