#

8.3 Disassembly and assembly of the Traverse Unit

TOP PREVIOUS NEXT

Step 1 Push the lever from position A to B.

Step 2 Pull the stopper (black) in the direction of arrow 1 and push the lever in the direction of arrow 2.

Step 3 Push the stopper (black) down until the white lever eject out.

Step 4 Lift up the traverse unit and slide out the unit as shown.

- Replacement of Traverse Unit

Step 1 Place the traverse unit as shown.

Step 2 Press in the lever shaft in the direction of arrow 1 as shown and push the traverse unit into the position in the direction of arrow 2.

Step 3 Pull the stopper in the direction of arrow 1 and release the lever in the direction of arrow 2 as shown.

Step 4 Pull out the tray half way and push it back fully.

Step 5 Push the lever to the initial position indicated ‘|---|’.

TOP PREVIOUS NEXT