#

9.2 Optical pickup adjustment

TOP PREVIOUS NEXT

Measurement point | Adjustment point | Mode | Test Disc
Service indicator on main unit | Tangential adjustment screw. Tilt adjustment screw. | Track 1 (Inner most circle) playback. Track 43 (Outer most circle) playback | DVD-S15 or DVDT-S01
Required equipment | Adjustment value
Hexagon wrench (Product No: JGS0100) Screw lock (Product No: RZZ0L01) | Adjust to minimum jitter value

Based on the diagram on the left.

1. When the jitter value changes as in A, the optimum point can be easily determined.

2. When the jitter value changes as in B, the optimum point is selected near the middle region.

TOP PREVIOUS NEXT