<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT65</Model>
<System>ORDER NO. MD0106136C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0706000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT65</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.6 Replacement of the Power IC</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0705000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0707000000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para>Carry out (Step 1) - (Step 3) in section 7.1</Para>
</item>
</randlist>
</Para>
<Para><emphasis>Step 1</emphasis>
 Cut out the connections located on the bottom cover. (6 points)</Para>
<Figure><graphic boardno="graphic36" reprowid="77.047mm" reprodep="76.539mm" location="internal"></Figure>
<Para><emphasis>[Caution]</emphasis>
 The bottom cover is reused after replacement . Take care, not to lose it.</Para>
<Figure><graphic boardno="graphic37" reprowid="80.257mm" reprodep="84.314mm" location="internal"></Figure>
<Para><emphasis>Step 2 </emphasis>
Bent the cut portion on the bottom cover.</Para>
<Figure><graphic boardno="graphic38" reprowid="80.772mm" reprodep="59.944mm" location="internal"></Figure>
<Para><emphasis>Step 3 </emphasis>
Remove solder on Power IC.</Para>
<Figure><graphic boardno="graphic39" reprowid="67.028mm" reprodep="51.153mm" location="internal"></Figure>
<Para><emphasis>[Caution]</emphasis>
</Para>
<Para><seqlist><item><Para>Apply compound grease (RFKX0002 or equivalent heat dissipating compound) on the rear face of the power IC when attaching Power IC.</Para>
</item>
<item><Para>Tighten adequately the 3 screws after replacement of Power IC.</Para>
</item>
<item><Para>Use the offset screwdriver for tightening and loosening of screws.</Para>
</item>
</seqlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0705000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0707000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
