#

15 Schematic Diagram

TOP PREVIOUS NEXT

(All schematic diagrams may be modified at any time with the development of the new technology)

Note:

- S621

  : Power On/Off switch

- S622

  : CD 1 switch

- S623

  : CD 2 switch

- S624

  : CD 3 switch

- S625

  : CD 4 switch

- S626

  : CD 5 switch

- S630

  : Open switch

- S631

  : Stop select switch

- S632

  : Pause select switch

- S633

  : Play select switch

- S634

  : Rev Skip switch

- S635

  : FWD Skip switch

- S636

  : Selector switch

- S637

  : Subwoofer Level switch

- SW1

  : Push switch

- SW2

  : Push switch

- SW3

  : Leaf switch

- SW4

  : CD switch

- SW5

  : Lock switch

- SW 2501

  : Leaf switch

- VR601

  : VR Volume Jog

- The voltage value and waveforms are the reference voltage of this unit measured by DC electronic voltmeter (high impedance) and oscilloscope on the basis of chassis. Accordingly, there may arise some error in voltage values and waveformsdepending upon the internal impedance of the tester or the measuring unit.

  No mark | : Playback | << >> | : Rec | < > | : FM
  (( )) | : CD | ( ) | : AM | [ ] | : AUX

- Importance safety notice :

  Components identified by mark have special characteristics important for safety. Furthermore, special parts which have purposes of fire-retardant (resistors), high-quality sound (capacitors), low-noise (resistors), etc. are used. Whenreplacing any of components, be sure to use only manufacturer´s specified parts shown in the parts list.

### Caution !

IC, LSI and VLSI are sensitive to static electricity.

Secondary trouble can be prevented by taking care during repair.

- Cover the parts boxes made of plastics with aluminium foil.

- Put a conductive mat on the work table.

- Ground the soldering iron.

- Do not touch the pins of IC, LSI or VLSI with fingers directly.

“CAUTION: REPLACE FUSIBLE RESISTOR WITH THE SAME TYPE RSFMB40KT-L FUSIBLE RESISTOR”“ATTENTION: REMPLACER LA RESISTANCE FUSIBLE PAR UNE RESISTENCE FUSIBLE DE MEME TYPE RSFMB40KT-L.

TOP PREVIOUS NEXT