<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT65</Model>
<System>ORDER NO. MD0106136C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0708000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT65</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.8 Disassembly and assembly of the Disc Tray</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0707000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0709000000
</nmlist>
</nameloc>
</Para>
<Figure><graphic boardno="graphic44" reprowid="89.239mm" reprodep="88.392mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
 With lifting the claw in the direction of arrow 1, draw the clamp SW P.C.B. in the direction of arrow 2.</Para>
<Para><emphasis>Step 3</emphasis>
 Remove the mechanism cover.</Para>
<Figure><graphic boardno="graphic45" reprowid="89.239mm" reprodep="82.169mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Insert the gear with hexagonal wrench into the hole.</Para>
<Figure><graphic boardno="graphic46" reprowid="74.253mm" reprodep="56.134mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
 Rotate the hexagonal wrench in the direction of arrow (clockwise), and then open the disc tray fully.</Para>
<Figure><graphic boardno="graphic47" reprowid="89.239mm" reprodep="83.651mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
 Upset the CD changer unit again.</Para>
<Para><emphasis>Step 7</emphasis>
 Release both the claws, and then draw the disc tray.</Para>
<Figure><graphic boardno="graphic48" reprowid="89.239mm" reprodep="85.598mm" location="internal"></Figure>
<Para><emphasis>Step 8</emphasis>
 With forcing the left guide bar manually because the left guide bar interfers with claw, draw the disc tray.</Para>
<Para><randlist prefix=unorder><item><Para><emphasis>Installation of the disc tray after replacement</emphasis>
</Para>
<Figure><graphic boardno="graphic49" reprowid="82.846mm" reprodep="62.527mm" location="internal"></Figure>
</item>
</randlist>
</Para>
<Para><emphasis>Step 1</emphasis>
 Slide the drive rack fully in the direction of arrow.</Para>
<Figure><graphic boardno="graphic50" reprowid="56.684mm" reprodep="81.196mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
 Holding the drive rack not to move, install the disc tray.</Para>
<Figure><graphic boardno="graphic51" reprowid="74.253mm" reprodep="85.175mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
 Align the drive rack with the driver gear.</Para>
<Figure><graphic boardno="graphic52" reprowid="84.455mm" reprodep="66.845mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Holding the disc tray manually, rotate the pulley gear in the direction of arrow.</Para>
<Para><emphasis>Step 5</emphasis>
 Rotate the gear 5 or 6 times manually, and then push the disc tray.</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0707000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0709000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
