#

10.4.1 Recovery after the DVD player is repaired

TOP PREVIOUS NEXT

When an FROM or an EEPROM in and on the module P.C.B. has replaced, carry out the recovery disc processing to optimize the drive.

Playback the disc above to process the recovery automatically.

Recovery disc (Product number: RFKZD5TR001 [SPC supply] )

FROM (Product number: RFKFRV45C040 [SPC supply] )

Note:

This unit requires no initialization process carried out after the traditional DVD players were repaired. When the recovery measures are taken, the customer setting will return to the factory setting as same as the procedure described in item of “Initialization:in 6.2 is carried out. Write down the contents of the setting before recovery processing, and reset the player.

TOP PREVIOUS NEXT