<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT65</Model>
<System>ORDER NO. MD0106136C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0709040000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT65</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.9.4 Assembly of Mechanised Drive Part</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0709030000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0710000000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>Step 1</emphasis>
 Install the traverse cam gear.</Para>
<Para><emphasis>Step 2</emphasis>
 Rotate the traverse cam gear fully in the clockwise direction.</Para>
<Figure><graphic boardno="graphic79" reprowid="91.017mm" reprodep="82.727mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
 Install the drive gear and traverse relay gear.</Para>
<Figure><graphic boardno="graphic80" reprowid="87.577mm" reprodep="80.786mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Unstall the slide plate (L) on the mechanised base and fit it to the connection lever.</Para>
<Para><emphasis>Step 5</emphasis>
 Install the slide plate (R) on the mechanised base. Fit it to the connection lever first before fitting the location with the trapezoidal tooth of the traverse relay gear.</Para>
<Figure><graphic boardno="graphic81" reprowid="85.196mm" reprodep="103.893mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
 Install the spindle base unit.(Install it first from the slide plate (R) side.</Para>
<Figure><graphic boardno="graphic82" reprowid="73.731mm" reprodep="71.967mm" location="internal"></Figure>
<Para><emphasis>Step 7</emphasis>
 Move the slide plate (R) fully to the front face side.</Para>
<Figure><graphic boardno="graphic83" reprowid="93.663mm" reprodep="69.850mm" location="internal"></Figure>
<Para><emphasis>Step 8</emphasis>
 Install the rear lock. (Ensure that tabs are engaged)</Para>
<Para><emphasis>Step 9</emphasis>
 Install the bottom SW board. (Ensure that the tabs are engaged).</Para>
<Figure><graphic boardno="graphic84" reprowid="86.894mm" reprodep="135.290mm" location="internal"></Figure>
<Para><emphasis>Step 11</emphasis>
 Detach tray lock spring from catch portion and hook it to the tray lock.</Para>
<Para><emphasis>Step 12</emphasis>
 Install the UP&sol;DOWN gear, change gear, gear changing spring, pulley gear and belt in the sequence of (1) ~ (5).</Para>
<Figure><graphic boardno="graphic85" reprowid="88.724mm" reprodep="71.614mm" location="internal"></Figure>
<Para><emphasis>Step 13</emphasis>
 Install the pitch plate and fix the screw (a).</Para>
<Figure><graphic boardno="graphic86" reprowid="72.849mm" reprodep="73.202mm" location="internal"></Figure>
<Para><emphasis>Step 13</emphasis>
 Install the disc tray, DVD traverse unit, mechanism cover, etc.</Para>
<Para><emphasis>[Confirm operation after completion)</emphasis>
</Para>
<Para>Rotate with the hexagon driver (gear) and confirm the operation of the following item.</Para>
<Para><seqlist><item><Para>Opening the disc tray.</Para>
</item>
<item><Para>Movement of trat towards stock side.</Para>
</item>
<item><Para>Up-Down movement of spindle base unit.</Para>
</item>
<item><Para>Up-Down movement of traverse unit.</Para>
</item>
</seqlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0709030000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0710000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
