<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT65</Model>
<System>ORDER NO. MD0106136C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0709020000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT65</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.9.2 Disassembly and assembly of Spindle Base Unit</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0709010000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0709030000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>Step 1</emphasis>
 Pull out 5 numbers of disc spacers after pressing down the bottom hook with a fine-tip minus screwdriver.</Para>
<Figure><graphic boardno="graphic64" reprowid="79.375mm" reprodep="81.139mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
 While pressing the tab, slide the support plate in direction of arrow and remove the support plate.</Para>
<Figure><graphic boardno="graphic65" reprowid="81.492mm" reprodep="49.918mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
 Pull out the disc lever with the disc lever turned in the direction of arrow (1).</Para>
<Figure><graphic boardno="graphic66" reprowid="90.488mm" reprodep="87.313mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Remove tab at 2 locations and pull out relay gear (B).</Para>
<Figure><graphic boardno="graphic67" reprowid="88.548mm" reprodep="79.552mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
 Remove tab at 2 locations.</Para>
<Figure><graphic boardno="graphic68" reprowid="90.664mm" reprodep="74.789mm" location="internal"></Figure>
<Figure><graphic boardno="graphic69" reprowid="70.909mm" reprodep="67.204mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
 Remove cushion spring.</Para>
<Para><emphasis>Step 7</emphasis>
 Remove rotation stopper (semi) in direction of arrow.</Para>
<Figure><graphic boardno="graphic70" reprowid="89.253mm" reprodep="98.073mm" location="internal"></Figure>
<Para><emphasis>Step 8</emphasis>
 Remove tab at 2 locations and pull out relay gear (A).</Para>
<Figure><graphic boardno="graphic71" reprowid="85.549mm" reprodep="48.860mm" location="internal"></Figure>
<Para><emphasis>Step 9</emphasis>
 Remove tab at 2 locations and detach the spindle shaft.</Para>
<Figure><graphic boardno="graphic72" reprowid="70.556mm" reprodep="36.513mm" location="internal"></Figure>
<Para><emphasis>Step 10</emphasis>
 Remove bottom spindle spring with a pair of tweezer.</Para>
<Figure><graphic boardno="graphic73" reprowid="88.500mm" reprodep="109.890mm" location="internal"></Figure>
<Para><emphasis>Step 11</emphasis>
 Press down the bottom hook with a fine-tip minus screwdriver.</Para>
<Para><emphasis>Step 12</emphasis>
 Hold the axis part of the bottom hook and pull it out.</Para>
<Figure><graphic boardno="graphic74" reprowid="90.664mm" reprodep="54.681mm" location="internal"></Figure>
<Para><emphasis>Step 13</emphasis>
 Turn the bottom spindle in the direction of arrow until it hits against the stopper.</Para>
<Para><emphasis>Step 14</emphasis>
 Insert a fine-tip minus screwdriver between the bottom spindle and UP&sol;DOWN base and slightly raise the bottom spindle for it to go over the stopper. Then turn the bottom spindle and remove it.</Para>
<Figure><graphic boardno="graphic75" reprowid="72.849mm" reprodep="38.100mm" location="internal"></Figure>
<Para><emphasis>Step 15</emphasis>
 Rotate the UP&sol;DOWN base 90&deg;. The spread the leg portion of the rotation stopper and remove the UP&sol;DOWN base.</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0709010000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0709030000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
