#

9.1 Preparation for adjustment

TOP PREVIOUS NEXT

1. Carry out STep 1 ~ Step 5 in Section 2 of Disassembly procedure and Major parts replacement procedure for operations check.

2. Remove the front panel and place it on a thick piece of paper on top of the main unit (Refer Fig. 1)

3. Prepare the service adjustment base and place the main unit on it. (Refer Fig. 1)

4. Adjust with hexagon wrench from bottom of service adjustment base (Refer Fig. 2 & 3)

Location of positioning adjustment screw

Bottom face of main unit (Front panel is detached)

TOP PREVIOUS NEXT