<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT65</Model>
<System>ORDER NO. MD0106136C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0000000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT65</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title id=cover>Service Manual</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0100000000x
</nmlist>
</nameloc>
</Para>
<Para>ORDER NO. MD0106136C1</Para>
<Para>A6</Para>
<Figure><graphic boardno="mttl1" location="internal"></Figure>
<Status><Subsystem>DVD Home Theatre Sound System</Subsystem>
<Figure><graphic boardno="logo1" location="internal"></Figure>
<Para><randlist prefix=simple><item><Para>SA-HT65</Para>
</item>
</randlist>
</Para>
<Para></Para>
<Para>Colour</Para>
<Para>(S)...  Silver Type</Para>
<Para></Para>
<Para>Area</Para>
<Para>(P)... U.S.A.</Para>
<Para></Para>
<Para>MECHANISM :</Para>
<Para>RAE1805Z-S TRAVERSE UNIT</Para>
</Status>
<Figure><graphic boardno="mdlpic2" reprowid="84.244MM" reprodep="43.773MM" location="internal"></Figure>
<Table frame="NONE" colsep="0" rowsep="0"><Title> Specifications</Title>
<tgroup cols="2" colsep="0" rowsep="0"><colspec colnum="1" colname="1" colwidth="1.752in" colsep="0">
<colspec colnum="2" colname="2" colwidth="1.733in" colsep="0">
<tbody><row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; AMPLIFIER SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>FTC TTL Power Output</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>240 W</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="JUSTIFY"><Para>120 Hz-20 kHz, 1.0&percnt; total harmonic distortion</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Front</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>30 W per channel (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Center</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>30 W (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Surround</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>30 W per channel (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="LEFT"><Para>45 Hz-120 Hz, 1.0&percnt; total harmonic distortion</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Subwoofer</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>90 W (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>RMS TTL Power Output</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>300 W</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="JUSTIFY"><Para>120 Hz - 20 kHz, 10&percnt; total harmonic distortion</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Front</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>36 W per channel (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Center</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>36 W (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Surround</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>36 W per channel (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="JUSTIFY"><Para>45 Hz - 120 Hz, 10&percnt; total harmonic distortion</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Subwoofer</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>120 W (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Input sensitivity&sol;input impedance</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>AUX</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>250 mV, 10 k&ohm; </Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; DISC SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Disc</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>DVD</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>8 cm&sol;12 cm Single-Side, SingleLayer</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>8 cm&sol;12 cm Single-Side, Double-Layer</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>8 cm&sol;12 cm Double-Side, Double- Layer</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>(One layer per side)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>CD&sol; VCD</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>8 cm&sol;12 cm (CD-R&sol;RW)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Video</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Signal system</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>NTSC</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Output level</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Composite video 1 Vp-p (75&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>S-video Y</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>1 Vp-p (75&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>S-video C</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>0.286 Vp-p (75&ohm;&sol;NTSC)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Audio</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Sampling frequency</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>CD</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>44.1 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>DVD</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>48 kHz&sol;96 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Decoding</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>16&sol;20&sol;24 bit linear</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Wow and flutter</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Below measurable limit</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>D&sol;A converter</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Delta-sigma DAC</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Pick up</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Beam Source</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Semiconductor Laser</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Wavelength</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>DVD</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>658 nm</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>VCD&sol;CD</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>790 nm</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; FM TUNER SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Frequency range</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>87.9-107.9 MHz (200 kHz steps)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>87.5-108.0 MHz (100 MHz steps)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Sensitivity</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>16.3 dBf (1.8&micro;V, IHF)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Antenna Terminals</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>75&ohm; unbalanced</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; AM TUNER SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Frequency range</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>520 - 1710 kHz (10 kHz steps)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Sensitivity</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>S&sol;N 20 dB at 1000 kHz</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>500&micro;V&sol;m</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; GENERAL</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Power supply</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>AC 120 V, 60 Hz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Power consumption</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>190 W</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Power consumption in standby mode</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>0.25 W</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Dimensions (W x H x D)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>430 x 114 x 368 mm</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>(16-15&sol;16&rdquo;x4-1&sol;2&rdquo;x14-1&sol;2&rdquo;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Mass</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>8.4 kg(18.5 Ib.)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; SYSTEM</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>SC-HT65 (P)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Main unit: SA-HT65 (P)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Speaker: SB-HT80A (P)</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="RIGHT"><Para>Sub woofer: SB-W70</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="RIGHT"><Para><emphasis>Notes:</emphasis>
</Para>
<Para><seqlist><item><Para>Specifiacations are subject to change without notice. Weight and dimensions are approximate.</Para>
</item>
<item><Para>Total harmonic distortion is measured by the digital spectrum analyzer.</Para>
</item>
</seqlist>
</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>&copy; 2001 Matsushita Electronics (S) Pte. Ltd. All rights reserved. Unauthorized copying and distribution is a violation of law.</Para>
<SafetyPara><Warning><Para><graphic boardno="graphic1" reprowid="183.000MM" reprodep="21.406MM" location="internal"></Para>
</Warning>
</SafetyPara>
<Figure><graphic boardno="bnm2" location="internal"></Figure>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0100000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
