#

10.2 DVD Self Diagnostic Function - Error Code

TOP PREVIOUS NEXT

Error Code | Error Content | Additional error explanation | Defect 1 | Defect 2 | Defect 3 | Defect 4
| U, H error |  |  |  |  |
U11 | Focus error |  |  |  |  |
H01 | Tray loading error |  |  |  |  |
H02 | Spindle servo error | (Spindle servo, DSC SP motor, CLV servo error) |  |  |  |
H03 | Traverse servo error |  |  |  |  |
H04 | Tracking servo error |  |  |  |  |
H05 | Seek error |  |  |  |  |
H06 | Power error | Cannot switch off the power because of the panel and system computer communication error |  |  |  |
| DSC related |  |  |  |  |
F500 | DSC error | DSC stops in the occurence of servo error (starup, focus error, etc) | OPU | ADSC | FEP | servo drive
F501 | DSC not Ready | DSC-system computer communication error (Communication failure caused by idling of DSC) | ADSC | CPU |  |
F502 | DSC Time out error | Similar disposal as F500 | OPU | ADSC | FEP | servo drive
F503 | DSC communication Failure | Communication error (result error occured although communication command was sent) | ADSC | FEP | EEPROM |
F505 | DSC Attention error | Similar disposal as F500 | OPU | ADSC | FEP | servo drive
F506 | Invalid media | Disc is flipped over, TOC unreadable, incompatible disc | DISC | FEP | ADSC | ODC
| ODC related |  |  |  |  |
F600 | Access failure to management information caused by demodulation error | Operation stopped because navigation data is not accessible caused by the demodulation defect | ODC | FEP | ADSC |
F601 | Indeterminate sector ID requested | Operation stopped caused by the request to access abnormal ID data | ODC | FEP | ADSC |
F602 | Access failure to LEAD-IN caused by demodulation error | LEAD IN data unreadable |  |  |  |
F603 | Access failure to KEYDET caused by demodulation error | Access failure to CSS data of disc |  |  |  |
F610 | ODC abnormality | No permission for command execution | ODC |  |  |
F611 | 6626 QCODE don’t read Error | Access failure to seek address in CD series | ODC |  |  |
F612 | No CRC OK for a specific time | Access failure to ID data in DVD series | ODC |  |  |
F630 | No reply to KEY DET enquiry | (for internal use only) |  |  |  |
F631 | CPPM KEY DET is not available till the FILE terminal | (CPPM file system is unreadable caused by scratches) | DISC | CPPM |  |
F632 | CPPM KEY DET is not available | Been revoked or falsified | DISC | EEPROM | CPPM |
| Disc code |  |  |  |  |
F103 | Illegal highlight Position | Big possibility of disc specification violation during highlight display | DISC |  |  |
| HIC Error |  |  |  |  |
F4FF | Force initialize failure (time out) |  | EEPROM | CPU | FEP | ADSC
| Micro computer error |  |  |  |  |
F700 | MBX overflow | When replying message to disc manager |  |  |  |
F701 | Message command does not end | Next message is sent before replying to disc manager |  |  |  |
F702 | Message command changes | Message is changed before it is sent as a reply to disc manager |  |  |  |
F880 | Task number is not appropriate | message coming from a non-existing task |  |  |  |
F890 | Sending message when message is being sent to AV task | Sending message to AV task |  |  |  |
F891 | Message couldn’t be sent to AV task | Begin sending message to AV task |  |  |  |
F893 | FROM falsification |  | FROM | CPU |  |
F894 | EEPROM abnormality |  | EEPROM | Serial communication on lone |  |
F8A0 | Message command is not appropriate | Begin sending message to AV task |  |  |  |

TOP PREVIOUS NEXT