#

10.1 Mode List

TOP PREVIOUS NEXT

Use this function when performing maintenance on the unit.

Main unit button | Remote control button | Usage
TUNE MODE | 0 | UHF display
5 | Positioning adjustment
6 | Confirmation of area code, transmission method
7 | Confirmation of internal program version
9 | Total illumination of main unit display panel
Screen Display | Confirmation of laser drive current
Pause | Saving of laser drive current value after optical pickup replacement (Do not perform this operation other than for replacement of optical pickup)
>10 | Initialisation of main unit (Return to factory shipment settings) Carry out for replacement of micro computer, peripheral parts of micro computer or printed board.

TOP PREVIOUS NEXT