<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT65</Model>
<System>ORDER NO. MD0106136C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1301000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT65</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>13.1 IC601 (C2BBGF000278) System Control</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1300000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1302000000
</nmlist>
</nameloc>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.623in">
<colspec colnum="2" colname="2" colwidth="0.702in">
<colspec colnum="3" colname="3" colwidth="0.400in">
<colspec colnum="4" colname="4" colwidth="1.700in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para><emphasis>Pin No.</emphasis>
</Para>
</entry>
<entry colname="2" align="center"><Para><emphasis>Mark</emphasis>
</Para>
</entry>
<entry colname="3" align="center"><Para><emphasis>I&sol;O</emphasis>
</Para>
</entry>
<entry colname="4" align="center"><Para><emphasis>Function</emphasis>
</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>D5_LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Disc 5 LED Control. Active H.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>D4_LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Disc 4 LED Control. Active H.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>D3_LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Disc 3 LED Control. Active H.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>D2_LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Disc 2 LED Control. Active H.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>D1_LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Disc 1 LED Control. Active H.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN or GND with Resistor</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY2</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 2 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY1</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 1 input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>9</Para>
</entry>
<entry colname="2" align="justify"><Para>JOG1B</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>JOG 1 INPUT B. Main Volume.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>10</Para>
</entry>
<entry colname="2" align="justify"><Para>JOG1A</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>JOG 1 INPUT A. Main Volume.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>11</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_VR</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>MIC VR AD input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>12</Para>
</entry>
<entry colname="2" align="justify"><Para>DSPRST</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>DSP reset output.Reset control for DSP micro computer.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>13</Para>
</entry>
<entry colname="2" align="justify"><Para>DSPACK</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>DSP ACK input. ACK input from DSP micro computer.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>14</Para>
</entry>
<entry colname="2" align="justify"><Para>SENSE</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>DSP sense input. SENSE input from DSP micro computer.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>15</Para>
</entry>
<entry colname="2" align="justify"><Para>PHONE</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>SW input for PHONE SW detection. L: without PHONE&sol;H:with PHONE</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>16</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC SW</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>SW input for MIC detection. L: without MIC&sol;H: with MIC</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>17</Para>
</entry>
<entry colname="2" align="justify"><Para>VSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>GROUND (VPP power input during FLASH)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>18</Para>
</entry>
<entry colname="2" align="justify"><Para>&sol;RESET</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Reset input. Active L.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>19</Para>
</entry>
<entry colname="2" align="justify"><Para>XCIN</Para>
</entry>
<entry colname="3" align="justify"><Para>L</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN or GND with Resistor</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>20</Para>
</entry>
<entry colname="2" align="justify"><Para>XCOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>L</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN or GND with Resistor</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>21</Para>
</entry>
<entry colname="2" align="justify"><Para>VSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>GROUND (0V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>22</Para>
</entry>
<entry colname="2" align="justify"><Para>XIN</Para>
</entry>
<entry colname="3" align="justify"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>4.00MHz Main Clock.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>23</Para>
</entry>
<entry colname="2" align="justify"><Para>XOUT</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>4.00MHz Main Clock.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>24</Para>
</entry>
<entry colname="2" align="justify"><Para>VCC</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power Supply. (&plus;5V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>25</Para>
</entry>
<entry colname="2" align="justify"><Para>MBP1</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN or GND with Resistor</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>26</Para>
</entry>
<entry colname="2" align="justify"><Para>MBP2</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN or GND with Resistor</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>27</Para>
</entry>
<entry colname="2" align="justify"><Para>PCONT</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>PCNT output. Power control output.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>28</Para>
</entry>
<entry colname="2" align="justify"><Para>DCDET</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>DCDET input. DC power detection input.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>29</Para>
</entry>
<entry colname="2" align="justify"><Para>RDS CLK</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>RDS clock input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>30</Para>
</entry>
<entry colname="2" align="justify"><Para>RDS DATA</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>RDS data input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>31</Para>
</entry>
<entry colname="2" align="justify"><Para>RMT</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>REMOCON input. Remote control input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>32</Para>
</entry>
<entry colname="2" align="justify"><Para>SYNC</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>AC failure DET input. Synchronized input for detection of power failure</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>33</Para>
</entry>
<entry colname="2" align="justify"><Para>SER4</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial 4 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>34</Para>
</entry>
<entry colname="2" align="justify"><Para>SER3</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial 3 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>35</Para>
</entry>
<entry colname="2" align="justify"><Para>SER2</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial 2 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>36</Para>
</entry>
<entry colname="2" align="justify"><Para>SER1</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial1 output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>37</Para>
</entry>
<entry colname="2" align="justify"><Para>SER 5</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Serial 5 output (ECHO CS)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>38</Para>
</entry>
<entry colname="2" align="justify"><Para>EDA</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM data output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>39</Para>
</entry>
<entry colname="2" align="justify"><Para>ECK</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM clock output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>40</Para>
</entry>
<entry colname="2" align="justify"><Para>ECS</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM CS output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>41</Para>
</entry>
<entry colname="2" align="justify"><Para>Dolby Digital LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Dolby Digital LED control</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>42</Para>
</entry>
<entry colname="2" align="justify"><Para>WAKE LED</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>WAKE UP display LED control. Active H</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>43</Para>
</entry>
<entry colname="2" align="justify"><Para>SD</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner signal DET input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>44</Para>
</entry>
<entry colname="2" align="justify"><Para>DO&sol;ST</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner DO&sol;ST input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>45</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>L output during TUNER</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>46</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM data input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>47-54</Para>
</entry>
<entry colname="2" align="justify"><Para>GRID8-GRID1</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Grid drive output(Digit drive output)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>55-72</Para>
</entry>
<entry colname="2" align="justify"><Para>SEG34-SEG17</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output (Anode drive output)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>73-80</Para>
</entry>
<entry colname="2" align="justify"><Para>SEG16-SEG9</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output (Anode drive output)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>81-88</Para>
</entry>
<entry colname="2" align="justify"><Para>SEG8-SEG1(REG8-REG1)</Para>
</entry>
<entry colname="3" align="justify"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Segment drive output (Anode drive output) Control output for regional area, function selection.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>89</Para>
</entry>
<entry colname="2" align="justify"><Para>VEE</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power jack</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>90</Para>
</entry>
<entry colname="2" align="justify"><Para>MECHSI</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mecha control data input (Communication with DVD mechanical controls</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>91</Para>
</entry>
<entry colname="2" align="justify"><Para>MECHSO</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mecha control data output (Communication with DVD mechanical controls</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>92</Para>
</entry>
<entry colname="2" align="justify"><Para>MECHCK</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mecha control clock intput (Communication with DVD mechanical controls</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>93</Para>
</entry>
<entry colname="2" align="justify"><Para>MECHRQ</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mecha con request output (Communication with DVD mechanical controls</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>94</Para>
</entry>
<entry colname="2" align="justify"><Para>MECHCS</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mecha control CS input (Communication with DVD mechanical controls</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>95</Para>
</entry>
<entry colname="2" align="justify"><Para>MECRST</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mechon reset output (Communication with DVD mechanical controls</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>96</Para>
</entry>
<entry colname="2" align="justify"><Para>REG_IN</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>Region input (Input setting for regional area, Function)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>97</Para>
</entry>
<entry colname="2" align="justify"><Para>AVSS</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power Jack (0V) AD Converter GROUND</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>98</Para>
</entry>
<entry colname="2" align="justify"><Para>VREF</Para>
</entry>
<entry colname="3" align="justify"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Reference power jack (&plus;5V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>99</Para>
</entry>
<entry colname="2" align="justify"><Para>N.C.</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>OPEN or GND with Resistor</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>100</Para>
</entry>
<entry colname="2" align="justify"><Para>CRT</Para>
</entry>
<entry colname="3" align="justify"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>CR timer control. Power failure time detection.</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
final
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1300000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1302000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
