#

9.1.1 Outline of Functions

TOP PREVIOUS NEXT

Selector | Complex Operation | Front Panel Display (Mode-in) | Next Operation | Test Content
DVD/CD | Main unit [STOP] Main unit [>>] | Y_ _ _ _ _ _ _ _ _ _ _ _ _ | [OPEN/CLOSE] | Changer mechanism operation; Self-Diagnostic code acquisition
[STOP] Single press | Display self-diagnostic code
[STOP] Long press | Clear recorded content of error conditions
Remote Control [5] | Changer mechanism continuous operation test
DVD/CD | Main unit [STOP] Remote Control [0] |  | None | Display DVD module self-diagnostic (Display error code)
Main unit [STOP] Other Remote Control button |  |  | Remote control [5] [6] [7] [9] [>=10] →[0]. [>=10] →[ENTER] [PAUSE] [DISPLAY] etc. Special commands for DVD module
Tuner | Main unit [STOP] Main unit [>>] | Button check display | All buttons | Button check, blink all front display panel lights
DVD/CD | Main unit [STOP] Main unit [>>] | T_ _ _ _ _ _ _ _ _ _ _ _ _ _ | [PAUSE] | Display analog device (AD) input value [ FF FF FF ] Front display panel (from left) [AN14] [AN15] [AN11]

### Cautions:

Self-diagnostics displayed via the [STOP] key display all recorded self-diagnostic codes.

TOP PREVIOUS NEXT