#

7.9.4 Assembly of Mechanised Drive Part

TOP PREVIOUS NEXT

Step 1 Install the traverse cam gear.

Step 2 Rotate the traverse cam gear fully in the clockwise direction.

Step 3 Install the drive gear and traverse relay gear.

Step 4 Unstall the slide plate (L) on the mechanised base and fit it to the connection lever.

Step 5 Install the slide plate (R) on the mechanised base. Fit it to the connection lever first before fitting the location with the trapezoidal tooth of the traverse relay gear.

Step 6 Install the spindle base unit.(Install it first from the slide plate (R) side.

Step 7 Move the slide plate (R) fully to the front face side.

Step 8 Install the rear lock. (Ensure that tabs are engaged)

Step 9 Install the bottom SW board. (Ensure that the tabs are engaged).

Step 11 Detach tray lock spring from catch portion and hook it to the tray lock.

Step 12 Install the UP/DOWN gear, change gear, gear changing spring, pulley gear and belt in the sequence of (1) ~ (5).

Step 13 Install the pitch plate and fix the screw (a).

Step 13 Install the disc tray, DVD traverse unit, mechanism cover, etc.

[Confirm operation after completion)

Rotate with the hexagon driver (gear) and confirm the operation of the following item.

1. Opening the disc tray.

2. Movement of trat towards stock side.

3. Up-Down movement of spindle base unit.

4. Up-Down movement of traverse unit.

TOP PREVIOUS NEXT