<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0903030000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>9.3.3 Jitter Offset Correction</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0903020000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0904000000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para>The jitter offset correction function below is necessary for D5, but is not necessary for D8.</Para>
</item>
<item><Para>While displaying K objects,certain remote control operations correct the offset of the DVD MODULE jitter value.</Para>
</item>
<item><Para>When the DVD module firmware rewriting connector is inserted K objects will be displayed [KC 00 0000].</Para>
</item>
<item><Para>Key codes of input from the remote control&rsquo;s ten key while displaying K objects are relayed to the system component by the operating console.</Para>
</item>
<item><Para>Inputting [2] [0] from the remote control returns a 14 hex value from the system component. The value is converted from hex &rarr; dec and displayed as [KC 20 0000].</Para>
</item>
<item><Para>Continuously pressing the [PLAY] button returns the offset result as a text string from the system component, which is displayed as [KC 20 0002].</Para>
</item>
<item><Para>The DVD Module has functions that support buttons other than [2] [0] [PLAY], so when K objects are being displayed key codes are as below.</Para>
<Para>[0] [1] [2] [3] [4] [5] [6] [7] [8] [9] [&gt;&equals;10] [PLAY]</Para>
</item>
</randlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0903020000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0904000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
