#

7.2.2 When opening manually

TOP PREVIOUS NEXT

Step 1 Insert the hexagon driver (gear bit) into the hole at the bottom face of the main body and turn it in the direction of the arow to open the disc tray.

Step 2 Release claw at 2 locations and remove tray trimming.

Step 3 After removing the tray trimming, push the disc tray back inside the main unit.

Step 5 Release claw at 2 locations and pull out the front panel.

- Carry out checks with Panel P.C.B. in the condition as indicated in diagram above.

Step 6 Over turn the DVD F/E module loading unit in the direction of arrow.

- Carry out checks with DSP P.C.B. and ASP P.C.B. in the condition as indicated in diagram below.

[Caution] Lay thick paper below the board.

TOP PREVIOUS NEXT