#

7.3 Checks for DVD Regulator P.C.B.

TOP PREVIOUS NEXT

- Carry out (Step 1) - (Step 3) in section 7.1

Step 2 Pull the tuner unit in direction of arrow(1). Disengage it from connector and remove in direction of arrow (2).

Step 3 Pull out FFC at CN805, CN806, CN1, CP6251 and CN1304.

Step 4 Detach DSP P.C.B. while removing tab on board holder.

Step 5 Connect back FFC at CN1, CP6251 and CN1304.

- Carry out checks with DVD Regulator P.C.B. in the condition as indicated in diagram below.

Step 6 Supply +5V from external power source to pin 10 terminal of connector (CP801) on main board.

TOP PREVIOUS NEXT