<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0702020000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.2.2 When opening manually</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0702010000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0703000000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>Step 1</emphasis>
 Insert the hexagon driver (gear bit) into the hole at the bottom face of the main body and turn it in the direction of the arow to open the disc tray.</Para>
<Figure><graphic boardno="graphic18" reprowid="66.887mm" reprodep="92.456mm" location="internal"></Figure>
<Figure><graphic boardno="graphic19" reprowid="64.382mm" reprodep="107.244mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
 Release claw at 2 locations and remove tray trimming.</Para>
<Para><emphasis>Step 3</emphasis>
 After removing the tray trimming, push the disc tray back inside the main unit.</Para>
<Figure><graphic boardno="graphic20" reprowid="72.849mm" reprodep="58.914mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
 Release claw at 2 locations and pull out the front panel.</Para>
<Figure><graphic boardno="graphic21" reprowid="64.516mm" reprodep="41.995mm" location="internal"></Figure>
<Para><randlist prefix=unorder><item><Para>Carry out checks with Panel P.C.B. in the condition as indicated in diagram above.</Para>
</item>
</randlist>
</Para>
<Figure><graphic boardno="graphic22" reprowid="66.887mm" reprodep="65.193mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
 Over turn the DVD F&sol;E module loading unit in the direction of arrow.</Para>
<Para><randlist prefix=unorder><item><Para>Carry out checks with DSP P.C.B. and ASP P.C.B. in the condition as indicated in diagram below.</Para>
</item>
</randlist>
</Para>
<Figure><graphic boardno="graphic23" reprowid="66.548mm" reprodep="62.653mm" location="internal"></Figure>
<Para><emphasis>[Caution]</emphasis>
 Lay thick paper below the board.</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0702010000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0703000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
