<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0705000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.5 Check for Power P.C.B.</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0704000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0706000000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para>Carry out (Step 1) - (Step 3) in section 7.1</Para>
</item>
<item><Para>Carry out (Step 1) - (Step 3) in section 7.4</Para>
</item>
</randlist>
</Para>
<Para><emphasis>Step 1</emphasis>
 Remove connector at CP705, CN503 and CN501.</Para>
<Figure><graphic boardno="graphic30" reprowid="87.313mm" reprodep="133.350mm" location="internal"></Figure>
<Figure><graphic boardno="graphic31" reprowid="87.207mm" reprodep="78.402mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
 Connect back connector at CN501 and CN503.</Para>
<Figure><graphic boardno="graphic32" reprowid="77.893mm" reprodep="91.271mm" location="internal"></Figure>
<Para><emphasis>Step 7</emphasis>
 Remove wire from connector CN102.</Para>
<Para><emphasis>Step 8</emphasis>
 Detach FFC at CN1, CP6251, CN1304 and CN806.</Para>
<Para><randlist prefix=unorder><item><Para>Carry out checks with Power P.C.B. in the condition as indicated in the diagram below.</Para>
</item>
</randlist>
</Para>
<Figure><graphic boardno="graphic33" reprowid="82.550mm" reprodep="69.321mm" location="internal"></Figure>
<Para><emphasis>Step 9</emphasis>
 Let the Main P.C.B. stand up.</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0704000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0706000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
