#

9.3.2 Special Commands for the DVD Module

TOP PREVIOUS NEXT

- When the SELECTOR is set to DVD/CD the commands for the operations below will be sent to the mechanism component micro-controller.

- The mechanism component micro-controller relays these commands without alteration to the DVD module.

- THe DVD module sends data resulting from commands to the mechanism component, where they are then relayed to the operating console.

- Data received from the DVD module by the operating console is displayed by the right 10 digits.

- Command Table

Special Operation | Command | Operation/Display | Release/Remarks
Jitter Display (servo test mode) | B5 | Main Unit [STOP] + Remote Control [5] xxx: jitter measurement (DEC) [xxx_yyy_zz] yyy:read error counter (DEC) zz: focus drive measurement (HEX) Test string from DVD MODULE:[J_xxx_yyy_zz] | Send STOP command from operating console
Region Display (location display) | B6 | Main Unit [STOP] + Remote Control [6] w: region number [_ _w_xy_zzz] x: N noPAL P PAL y: N NTSC 6 PAL60 zzz: panel component jumper data Text string from DVD MODULE:[_ _w_xy_zzz] | 5 seconds after activation the text string from the DVD MODULE dissappears and display is automatically turned off.
Version Display | B7 | Main Unit [STOP] = Remote Control [7] s: panel component mode type [srrrxxyzzz] rrr: panel component release number [_ _ _xxyzzz] x: generation of system component (45) y:system component model type zzz: system component release number Text string from DVD MODULE: [srrr_ _xxyzzz] srrr will be blank with mini-components | 5 seconds after activation the text string from the DVD MODULE dissappears and display is automatically turned off.
Error Code Display | BA + request record number | Main Unit [STOP] + Remote Control [0] [__DVD_Fxxx] xxx: error number [__DVD_Uxxx] [__DVD_Hxxx] | 5 seconds after activation the text string from the DVD MODULE dissappears and display is automatically turned off.
Laser Current Initial measurement (saved laser power value) | C2 | Main Unit [STOP] + Remote Control [PAUSE] [DO_034_028] 034: DVD current measurement (mA) (DEC) 028: CD current measurement (mA) (DEC) Text string from DVD MODULE: [LDO_034_028] |
DVD Laser Current Measurement | C3 | Main Unit [STOP] + Remote Control [DISPLAY] 034: saved in EEPROM [DD_034_032] initial current mearement (mA) (DEC) 032: present current measurement (mA) (DEC) Text stringfrom DVD MODULE: [LDD_034_032] | Laser lighting remains on until POWER OFF of the tray opens.
ADSC Internal RAM Display A | C4 | Main Unit [STOP] + Remote Control [1] [A_0FA_6901] 0FA: address (HEX) 6901: RAM value of display address (HEX) | STOP command is sent from the operating console to the DVD MODULE
ADSC Internal RAM Display B | C5 | Main Unit [STOP] + Remote Control [2] [A_0FA_6901] 0FA: address (HEX) 6901: RAM value of display address (HEX) | STOP command is sent from the operating console to the DVD MODULE
kink measurement (invalid pick detection) | C6 | Main Unit [STOP] + Remote Control [9] [FK_109_101] 109: maximum value of calculated value (DEC) 101 : ratio of maximum value to minimum value [FK_ER_9101] ER: display error occurance 9101:ADSC command error code | STOP command is sent from the operating console to the DVD MODULE
User Initialization (For users) | BC+ Model Table + 0 x 00 | Main Unit [STOP] + Remote Control [>=10] [INITIALIZED] display on the operating console for 2 seconds. When display clears the user initialization commands is output thesystem component. Returns user settings to factory values. | When the [INITIALIZED] on the front panel dissappears the operation is complete. to GUI is INITIALIZE.
All Reset (for design service) | BC+ Model Table + 0 x 3C | While [INITIALIZED] is being displayed from the user initialization operation press [STOP] on the main unit and [ENTER] on the remote control. [_DVD_RESET] is displayed on the operatingconsole and the all reset command is output instead of the user initialization command. Returns user settings to factory values. Panel component jumpers are referenced, and the appropriate model number’s initialization valuesare written to the EEPROM and global region. Laser times and spindle times are not initialized. | If NO DISC or ---READ can be confirmed after DVD RESET is displayed on the front display panel the operation is completed.
No GUI. All items temporarily dissappear.
All set (for industrial production) | F1 | Receipt of remote control code [B0 00 F1]. Also, Main Unit [STOP] + Remote Control [1DDF] [_ALL_SET] (display text string from system component). Returns user settings to factoryvalues. Panel component jumpers are referenced, and the appropriate model number’s initialization values are written to the EEPROM and the global region. Laser times and spinlde times are also initialized. | If NO DISC or ---READ can be confirmed after ALL SET is displayed on the front display panel the operation is completed. ALL SET is displayed on the front displaye panel the operationis completed. GUI is ALL SET.
Device Name Display | B1+ 0 x 13 | Main Unit [STOP] + Remote Control [4] [FEP_??????] [SRV_??????] [ODC_??????] [Av_??????] [SYS_??????] | Display cycles every 3 seconds. Display automatically turns off after the last device name is displayed.
Laser Time Use | B1+ 0 x 14 | Main Unit [STOP] + Remote Control [^] 1234 : DVD laser use time [_1234_5678] 5678: CD laser use time 10 hour units displayed in 4 digits Text string from DVD MODULE: [T1_1234_5678] | 5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.
Reset Laser Time Use | B2 + 0 x 14 | While use time is being displayed press Main Unit [STOP] + Remote Control [V] [_0000_0000] DVD and CD are both reset at the same time. | 5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.
Spindle Use Time | B1 + 0 x 15 | Main Unit [STOP] + Remote Control [>] [___T2_1234] 1234: 10 hour units displayed in 4 digits Text string from DVD MODULE: [T2_1234_____] | 5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.
Reset Spindle Use Time | B2 + 0 x 15 | While use time is being displayed press Main Unit [STOP] + Remote Control [<] [___T2_0000] | 5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.
CD Laser Current Measurement | B1 + 0 x 92 | Main Unit [STOP] + Remote Control [3] 028: initial current value [DC_028_026] stored in EEPROM (mA) 026: Present current value (mA) Text string from DVD MODULE: [LDG_028_026] | Laser lighting continues until POWER OFF or the tray opens.
Region and Firmware Version Display | BF + 0 x 92 | Main Unit [STOP] + Remote Control [8] r: region number [__r__xyzzz] x: generation of system component y: system component model type zzz: system component model type Textstring from DVD MODULE: [____r__xyzzz] | 5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.
Transmission Error Display | BF + 0 x 11 | Main Unit [STOP] + Remote Control [MENU] [_ERR_02/30] | 5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.

TOP PREVIOUS NEXT