<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0903010000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>9.3.1 Tray Lock Function</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0903000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0903020000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para>There are two tray lock functions</Para>
</item>
<item><Para>Power on through the SELECTOR &sol;DVD&sol;CD. While holding down the [CD STOP] button on the main unit press the [POWER] button on the main unit or the remote control. Lock Mode A will be entered, [_ _ _ _LOCKED_ _] will be displayedfor 3 seconds, and the current disc will begin playing.</Para>
</item>
<item><Para>Lock Mode A will disable the button below while turning the power on or off.</Para>
<Para>[OPEN&sol;CLOSE]</Para>
</item>
<item><Para>When  locked in Lock Mode A pressing the [POWER] button on the main unit or the remote control while holding down the [CD STOP] button on the main unit will display [_ _UNLOCKED_ _] and unlock the unit.</Para>
</item>
<item><Para>Power on through the SELECTOR DVD&sol;CD. While holding down the [CD PLAY] button on the main unit press the [POWER] button on the main unit or the remote control. Lock Mode B will  be entered, [_ _ _LOCKED_ _] will be displayed for 3 seconds,and the current disc will begin playing.</Para>
</item>
<item><Para>In Lock Mode B the button below, mainly selector and disc operation related items, will be disabled.</Para>
<Para>Main Unit: [OPEN&sol;CLOSE] [PAUSE] [STOP] [I&lt;&lt;&sol;V] [SELECTOR] [DISK SKIP]</Para>
<Para>Remote Control: [AUX] [DVD&sol;CD] [TV] [VCR] [TUNER&sol;BAND] [0] ~ [9] [&gt;&equals;10] [DISK]</Para>
<Para>                           [I&lt;&lt;] [I&gt;&gt;] [PAUSE] [STOP] [&lt;&lt;] [&gt;&gt;] [REPEAT] [POSITION]</Para>
<Para>                           [A-B REPEAT] [MARKER] [DISPLAY] [MIX2ch] [TEST] [TIMER] [FL DISPLAY] [CH SELECT]</Para>
<Para>                           [KARAOKE ON&sol;OFF] [KARAOKE DISPLAY] [VOICE] [MUTE]</Para>
<Para>                           [ECHO] [b] [&num;] [CENTER FOCUS] {SEAT POSITION] [RETURN] [DISK SKIP]</Para>
<Para>                           [CINEMA] [GROUP] [PAGE]</Para>
<Para>While playing it is not necessary to re-disable buttons disabled under Lock Mode B.</Para>
<Para>Also, button related to sound quality are not disabled. The buttons below are not disabled.</Para>
<Para>Main Unit: [POWER]</Para>
<Para>Remote Control: [POWER] [DISK MANAGER] [PALY MODE] [CANCEL] [SFC] [SUBWOOFER LEVEL]</Para>
<Para>                           [VOL-] [VOL&plus;] [SUPER SURROUND] [DOLBY PROLOGIC] [SUB TITLE] [AUDIO] [ANGLE]</Para>
<Para>                           [TOP MENU] [MENU] [ENTER] [&lt;] [&gt;] [^] [V] [MUTING] [PLAY]</Para>
</item>
<item><Para>When locked in Lock Mode B pressing the [POWER] button on the main unit or the remote control while holding down the [CD PLAY] button on the main unit will unlock the unit after displaying [_ _UNLOCKED_ _] for 3 seconds.</Para>
</item>
<item><Para>Tray lock is canceled when AC power is cut.</Para>
</item>
<item><Para>Tray lock A and B functions are exclusive operations. The first one enabled will have priority.</Para>
</item>
<item><Para>In Lock Mode A any selector button is allowed to start auto power on.</Para>
<Para>In Lock Mode B all selector buttons are disable from starting auto power on.</Para>
</item>
<item><Para>When a disabled button is pressed while in lock mode [_ _ _LOCKED_ _] will be displayed for 3 seconds on the front display panel.</Para>
</item>
<item><Para>Lock mode will be cancelled when a loading error occurs with the CR20.</Para>
<Para>(If the [OPEN&sol;CLOSE] button were disabled when the tray is opened by a TAKE OUT DISC error recovery would be impossible)</Para>
</item>
</randlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0903000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0903020000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
