<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0903020000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>9.3.2 Special Commands for the DVD Module</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0903010000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0903030000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para>When the SELECTOR is set to DVD&sol;CD the commands for the operations below will be sent to the mechanism component micro-controller.</Para>
</item>
<item><Para>The mechanism component micro-controller relays these commands without alteration to the DVD module.</Para>
</item>
<item><Para>THe DVD module sends data resulting from commands to the mechanism component, where they are then relayed to the operating console.</Para>
</item>
<item><Para>Data received from the DVD module by the operating console is displayed by the right 10 digits.</Para>
</item>
<item><Para>Command Table</Para>
</item>
</randlist>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="1.009in">
<colspec colnum="2" colname="2" colwidth="0.940in">
<colspec colnum="3" colname="3" colwidth="3.110in">
<colspec colnum="4" colname="4" colwidth="2.051in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>Special Operation</Para>
</entry>
<entry colname="2" align="center"><Para>Command</Para>
</entry>
<entry colname="3" align="center"><Para>Operation&sol;Display</Para>
</entry>
<entry colname="4" align="center"><Para>Release&sol;Remarks</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>Jitter Display</Para>
<Para>(servo test mode)</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B5</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [5]</Para>
<Para>xxx: jitter measurement (DEC)</Para>
<Para>[xxx_yyy_zz]   yyy:read error counter (DEC)</Para>
<Para>zz: focus drive measurement (HEX)</Para>
<Para>Test string from DVD MODULE:[J_xxx_yyy_zz]</Para>
</entry>
<entry colname="4" align="justify"><Para>Send STOP command from operating console</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Region Display</Para>
<Para>(location display)</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B6</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [6]</Para>
<Para>w: region number</Para>
<Para>[_ _w_xy_zzz]  x: N noPAL P PAL</Para>
<Para>y: N NTSC 6 PAL60</Para>
<Para>zzz: panel component jumper data</Para>
<Para>Text string from DVD MODULE:[_ _w_xy_zzz]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappears and  display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Version Display</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B7</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &equals; Remote Control [7]</Para>
<Para>s: panel component mode type</Para>
<Para>[srrrxxyzzz]   rrr: panel component release number</Para>
<Para>[_ _ _xxyzzz]  x: generation of system component (45)</Para>
<Para>y:system component model type</Para>
<Para>zzz: system component release number</Para>
<Para>Text string from DVD MODULE: [srrr_ _xxyzzz]</Para>
<Para>srrr will be blank with mini-components</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappears and  display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Error Code Display</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>BA &plus; </Para>
<Para>request</Para>
<Para>record</Para>
<Para>number</Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [0]</Para>
<Para>[__DVD_Fxxx]   xxx: error number</Para>
<Para>[__DVD_Uxxx]</Para>
<Para>[__DVD_Hxxx]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappears and  display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Laser Current</Para>
<Para>Initial measurement</Para>
<Para>(saved laser power value)</Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>C2</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [PAUSE]</Para>
<Para>[DO_034_028] 034: DVD current measurement (mA) (DEC)</Para>
<Para>028: CD current measurement (mA) (DEC)</Para>
<Para>Text string from DVD MODULE: [LDO_034_028]</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>DVD Laser</Para>
<Para>Current Measurement</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>C3</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [DISPLAY]</Para>
<Para>034: saved in EEPROM</Para>
<Para>[DD_034_032]   initial current mearement (mA) (DEC)</Para>
<Para>032: present current measurement (mA) (DEC)</Para>
<Para>Text stringfrom DVD MODULE: [LDD_034_032]</Para>
</entry>
<entry colname="4" align="justify"><Para>Laser lighting  remains on until POWER OFF of the tray opens.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>ADSC</Para>
<Para>Internal RAM Display A</Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>C4</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [1]</Para>
<Para>[A_0FA_6901] 0FA: address (HEX)</Para>
<Para>6901: RAM value of display address (HEX)</Para>
</entry>
<entry colname="4" align="justify"><Para>STOP command is sent from the operating console to the DVD MODULE</Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>ADSC</Para>
<Para>Internal RAM Display B</Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>C5</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [2]</Para>
<Para>[A_0FA_6901] 0FA: address (HEX)</Para>
<Para>6901: RAM value of display address (HEX)</Para>
</entry>
<entry colname="4" align="justify"><Para>STOP command is sent from the operating console to the DVD MODULE</Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>kink measurement</Para>
<Para>(invalid pick detection)</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>C6</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [9]</Para>
<Para>[FK_109_101]   109: maximum value of calculated value (DEC)</Para>
<Para>101 : ratio of maximum value to minimum value</Para>
<Para>[FK_ER_9101] ER: display error occurance</Para>
<Para>9101:ADSC command error code</Para>
</entry>
<entry colname="4" align="justify"><Para>STOP command is sent from the operating console to the DVD MODULE</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>User Initialization</Para>
<Para>(For users)</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify">BC&plus; <Para>Model Table</Para>
<Para>&plus; 0 x 00</Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [&gt;&equals;10]</Para>
<Para>[INITIALIZED] display on the operating console for 2 seconds.</Para>
<Para>When display clears the user initialization commands is output thesystem component.</Para>
<Para>Returns user settings to factory values.</Para>
</entry>
<entry colname="4" align="justify"><Para>When the [INITIALIZED] on the front panel dissappears the operation is complete.</Para>
<Para></Para>
<Para>to GUI is INITIALIZE.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" morerows="1" align="justify"><Para>All Reset</Para>
<Para>(for design service)</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" morerows="1" align="justify"><Para>BC&plus; </Para>
<Para>Model Table</Para>
<Para>&plus; 0 x 3C</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" morerows="1" align="justify"><Para>While [INITIALIZED] is being displayed from the user initialization operation press [STOP] on the main unit and [ENTER] on the remote control.</Para>
<Para>[_DVD_RESET] is displayed on the operatingconsole and the all reset command is output instead of the user initialization command.</Para>
<Para>Returns user settings to factory values.</Para>
<Para>Panel component jumpers are referenced, and the appropriate model number&rsquo;s initialization valuesare written to the EEPROM and global region.</Para>
<Para>Laser times and spindle times are not initialized.</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
<Para>If NO DISC or ---READ can be confirmed after DVD RESET is displayed on the front display panel the operation is completed.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="4" align="justify"><Para>No GUI. All items temporarily dissappear.</Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>All set</Para>
<Para>(for industrial production)</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>F1</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Receipt of remote control code [B0 00 F1].</Para>
<Para>Also, Main Unit [STOP] &plus; Remote Control [1DDF]</Para>
<Para>[_ALL_SET] (display text string from system component).</Para>
<Para>Returns user settings to factoryvalues.</Para>
<Para>Panel component jumpers are referenced, and the appropriate model number&rsquo;s initialization values are written to the EEPROM and the global region.</Para>
<Para>Laser times and spinlde times are also initialized.</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
<Para></Para>
<Para>If NO DISC or ---READ can be confirmed after ALL SET is displayed on the front display panel the operation is completed.</Para>
<Para>ALL SET is displayed on the front displaye panel the operationis completed.</Para>
<Para>GUI is ALL SET.</Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Device Name Display</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B1&plus; </Para>
<Para>0 x 13</Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [4]</Para>
<Para>[FEP_??????] [SRV_??????] [ODC_??????]</Para>
<Para>[Av_??????] [SYS_??????]</Para>
</entry>
<entry colname="4" align="justify"><Para>Display cycles every 3 seconds. Display automatically turns off after the last device name is displayed.</Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Laser Time Use</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B1&plus; </Para>
<Para>0 x 14</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [^]</Para>
<Para>1234 : DVD laser use time</Para>
<Para>[_1234_5678] 5678: CD laser use time</Para>
<Para>10 hour units displayed in 4 digits</Para>
<Para>Text string from DVD MODULE: [T1_1234_5678]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Reset Laser Time Use</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B2 &plus; </Para>
<Para>0 x 14</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>While use time is being displayed press</Para>
<Para>Main Unit [STOP] &plus; Remote Control [V]</Para>
<Para>[_0000_0000]</Para>
<Para>DVD and CD are both reset at the same time.</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Spindle Use Time</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B1 &plus; </Para>
<Para>0 x 15</Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [&gt;]</Para>
<Para>[___T2_1234] 1234: 10 hour units displayed in 4 digits</Para>
<Para>Text string from DVD MODULE: [T2_1234_____]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Reset Spindle Use Time</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B2 &plus; </Para>
<Para>0 x 15</Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>While use time is being displayed press</Para>
<Para>Main Unit [STOP] &plus; Remote Control [&lt;]</Para>
<Para>[___T2_0000]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>CD Laser Current Measurement</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>B1 &plus; </Para>
<Para>0 x 92</Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [3]</Para>
<Para>028: initial current value</Para>
<Para>[DC_028_026]  stored in EEPROM (mA)</Para>
<Para>026: Present current value (mA)</Para>
<Para>Text string from DVD MODULE: [LDG_028_026]</Para>
</entry>
<entry colname="4" align="justify"><Para>Laser lighting continues until POWER OFF or the tray opens.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>Region and Firmware Version Display</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>BF &plus; </Para>
<Para>0 x 92</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [8]</Para>
<Para>r: region number</Para>
<Para>[__r__xyzzz]  x: generation of system component</Para>
<Para>y: system component model type</Para>
<Para>zzz: system component model type</Para>
<Para>Textstring from DVD MODULE: [____r__xyzzz]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.</Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
<Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>Transmission Error Display</Para>
<Para></Para>
</entry>
<entry colname="2" align="justify"><Para>BF &plus; </Para>
<Para>0 x 11</Para>
</entry>
<entry colname="3" align="justify"><Para>Main Unit [STOP] &plus; Remote Control [MENU]</Para>
<Para>[_ERR_02&sol;30]</Para>
</entry>
<entry colname="4" align="justify"><Para>5 seconds after activation the text string from the DVD MODULE dissappear and display is automatically turned off.</Para>
<Para></Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0903010000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0903030000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
