<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0902000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>9.2 Self-Diagnostic Mode Settings and Display</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0901010000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0903000000
</nmlist>
</nameloc>
</Para>
<Para><seqlist><item><Para>Power-source related</Para>
<Para>&ast; Example display</Para>
<Figure><graphic boardno="graphic95" reprowid="69.258mm" reprodep="14.055mm" location="internal"></Figure>
<Para>&ast; Self-Diagnostic Codes</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.792in">
<colspec colnum="2" colname="2" colwidth="1.122in">
<colspec colnum="3" colname="3" colwidth="2.606in">
<colspec colnum="4" colname="4" colwidth="2.502in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>No.</Para>
</entry>
<entry colname="2" align="center"><Para>Error Display</Para>
</entry>
<entry colname="3" align="center"><Para>Error Item</Para>
</entry>
<entry colname="4" align="center"><Para>Detection Method</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="0"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>F61</Para>
</entry>
<entry colname="3" align="justify"><Para>Power Amp output error or power supply circuit error</Para>
</entry>
<entry colname="4" align="justify"><Para>When DCDET is L during normal operation do not POWER OFF normally, immediately set PCNT to L and display F61 error.Do not start demonstrations while error F61 is being displayed.Record content of error occuranceand display content in error detection mode.</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
</item>
<item><Para>CD&sol;DVD Changer Mechanism (CR20)</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.792in">
<colspec colnum="2" colname="2" colwidth="2.882in">
<colspec colnum="3" colname="3" colwidth="3.450in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>Step</Para>
</entry>
<entry colname="2" align="center"><Para>Operating Procedure</Para>
</entry>
<entry colname="3" align="center"><Para>Micro-controller operation, processing, etc.</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>Switch the SELECTOR to CD&sol;DVD, close tray without disk</Para>
</entry>
<entry colname="3" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>Press the [FF] button while holding down the [STOP] button for two seconds or more. Self-diagnostic mode is entered when the [STOP] button is released.</Para>
</entry>
<entry colname="3" align="justify"><Para>Self-diagnostic mode will not be entered if there is a disk in the tray.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>[T            ] is displayed by the front display (FL) panel when entering self-diagnostic mode.</Para>
</entry>
<entry colname="3" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>Press the [OPEN&sol;CLOSE] button.</Para>
</entry>
<entry colname="3" align="justify"><Para>Operations below will be continued. While operations are in progress buttons relating to the micro-controller will be ignored.</Para>
<Para><seqlist><item><Para>Change disc 1 and open the tray.</Para>
</item>
<item><Para>Close the tray 1 second after opening.</Para>
</item>
<item><Para>Initialize the mechanism.</Para>
</item>
<item><Para>Insert disc 5 in the play position and quit.</Para>
</item>
</seqlist>
</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>Confirm recorded error content by pressing the [STOP] button while stopped in the self-diagnostic mode and displaying the results of the error check.</Para>
</entry>
<entry colname="3" align="justify"><Para>Each time the [STOP] button is pressed error item codes are displayed in sequence on the front display panel Example of a DVD module content display: [_DVD_H05_ _]Example of a normal self diagnostic code display:[T_ _ _H02_ _]</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>Clear recorded error content by pressing the [STOP] button for 5 seconds or more while stopped in the self-diagnostic mode.</Para>
</entry>
<entry colname="3" align="justify"><Para>Recorded error content is cleared and the following is shown on the front display panel:[CLEAR] is displayed for one second followed by a return to [T_ _ _ _ _ _ _]</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>Cancel self-diagnostic mode by pressing the [POWER] button.</Para>
</entry>
<entry colname="3" align="justify"><Para>Power is turned off. At the next power on normal operation will resume.</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>&ast; If an error occurs while checking the RAM during a micro-controller reset all recorded error detection content will be cleared while initializing the RAM.</Para>
<Para>&ast; By skipping step 4 of the above procedure and moving directly to step 6 it is possible to just display the self-diagnostic codes.</Para>
<Para>&ast; Example display</Para>
<Figure><graphic boardno="graphic96" reprowid="68.749mm" reprodep="14.055mm" location="internal"></Figure>
<Para>&ast; Self-Diagnostic Codes</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.792in">
<colspec colnum="2" colname="2" colwidth="1.122in">
<colspec colnum="3" colname="3" colwidth="1.770in">
<colspec colnum="4" colname="4" colwidth="3.210in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>No.</Para>
</entry>
<entry colname="2" align="center"><Para>Error Display</Para>
</entry>
<entry colname="3" align="center"><Para>Error Item</Para>
</entry>
<entry colname="4" align="center"><Para>Detection Method</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>H15</Para>
</entry>
<entry colname="3" align="justify"><Para>OPEN SW error</Para>
</entry>
<entry colname="4" align="justify"><Para>If there is a failsafe for a SW error that occurs during normal operation it will be recorded and displayed in self-diagnostic mode.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>H16</Para>
</entry>
<entry colname="3" align="justify"><Para>CLOSE SW error</Para>
</entry>
<entry colname="4" align="justify"><Para>SW errors will be detected even in error detection mode.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>H16</Para>
</entry>
<entry colname="3" align="justify"><Para>UP SW error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>H17</Para>
</entry>
<entry colname="3" align="justify"><Para>DOWN SW error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>H27</Para>
</entry>
<entry colname="3" align="justify"><Para>POSITION SW error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>F28</Para>
</entry>
<entry colname="3" align="justify"><Para>DISC mount error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>F29</Para>
</entry>
<entry colname="3" align="justify"><Para>DISC unmount error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>&ast; While stopped in conditions 3 or higher above it is possible to start a CR20 continuous test. Described in detail seperately.</Para>
</item>
<item><Para>Analog Device (AD) input value display</Para>
<Para>&ast; Pressing the [PAUSE] button on the main unit after having entered self-diagnostic mode through SELECTOR [DVD&sol;CD] will show the analog device conversion input value on the front display panel. </Para>
<Para>&ast; Each time the button is pressed the value will be read again and the display refreshed.</Para>
<Para>&ast; Front display Panel:</Para>
<Figure><graphic boardno="graphic97" reprowid="73.491mm" reprodep="30.988mm" location="internal"></Figure>
<Para><emphasis>Note:</emphasis></Para>
<Para>Empty entries will displays as &ldquo;00&rdquo;.</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="2" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="1.861in">
<colspec colnum="2" colname="2" colwidth="4.981in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>AD Input</Para>
</entry>
<entry colname="2" align="center"><Para>Usage</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>AN 14</Para>
</entry>
<entry colname="2" align="justify"><Para>Key 1 input : Key input 1</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>AN 15</Para>
</entry>
<entry colname="2" align="justify"><Para>Key 2 input : Key input 2</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>AN 11</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_VR input: MIC VR input</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para><randlist prefix=unorder><item><Para>Exit the Analog Device input value display mode by cutting off the AC power source and next time could start the device.</Para>
</item>
</randlist>
</Para>
</item>
<item><Para>DVD&sol;CD module </Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.792in">
<colspec colnum="2" colname="2" colwidth="2.882in">
<colspec colnum="3" colname="3" colwidth="3.450in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>Step</Para>
</entry>
<entry colname="2" align="center"><Para>Operating Procedure</Para>
</entry>
<entry colname="3" align="center"><Para>Micro-controller operation, processing, etc.</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>Set the SELECTOR to CD&sol;DVD</Para>
</entry>
<entry colname="3" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>While pressing the [STOP] button on the main unit press [0] button on the remote control</Para>
</entry>
<entry colname="3" align="justify"><Para>See the &ldquo;DVD&sol;CD&sol; Changer Control&rdquo; section of &ldquo;Error Display&rdquo; for a detailed explanation.</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>&ast; Since error detection for the DVD&sol;CD module occurs in the system component and is sent through the mechanism component codes are received and displayed at the operating console.</Para>
<Para>&ast; Since self-diagnostic codes for the DVD&sol;CD module duplicate prior audio codes the self-diagnostic codes are displayed prefixed by &ldquo;DVD&rdquo;.</Para>
<Figure><graphic boardno="graphic98" reprowid="70.273mm" reprodep="14.055mm" location="internal"></Figure>
<Para>&ast; Self-Diagnostic Codes</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.792in">
<colspec colnum="2" colname="2" colwidth="1.122in">
<colspec colnum="3" colname="3" colwidth="2.606in">
<colspec colnum="4" colname="4" colwidth="2.502in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>No.</Para>
</entry>
<entry colname="2" align="center"><Para>Error Display</Para>
</entry>
<entry colname="3" align="center"><Para>Error Explanation</Para>
</entry>
<entry colname="4" align="center"><Para>Cause (IC number, etc.)</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>F010</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than the specified parental value.</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>F020</Para>
</entry>
<entry colname="3" align="justify"><Para>No TT_SRPT (RLBN is 0)</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>F021</Para>
</entry>
<entry colname="3" align="justify"><Para>TT_SRP number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>F022</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than the TT_SRP number</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>F023</Para>
</entry>
<entry colname="3" align="justify"><Para>No matching SRP for VTSN or VTS_TTN</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>F024</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than TT_SRP.PTT_Ns</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>F030</Para>
</entry>
<entry colname="3" align="justify"><Para>TTU_SRP number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>F031</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than TTU_SRP number</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>9</Para>
</entry>
<entry colname="2" align="justify"><Para>F040</Para>
</entry>
<entry colname="3" align="justify"><Para>SRP1 number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>10</Para>
</entry>
<entry colname="2" align="justify"><Para>F041</Para>
</entry>
<entry colname="3" align="justify"><Para>PGCI_SRP number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>11</Para>
</entry>
<entry colname="2" align="justify"><Para>F042</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than the PGCI_SRP number</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>12</Para>
</entry>
<entry colname="2" align="justify"><Para>F043</Para>
</entry>
<entry colname="3" align="justify"><Para>No matching PGCI_SRP for this Menu ID</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>13</Para>
</entry>
<entry colname="2" align="justify"><Para>F050</Para>
</entry>
<entry colname="3" align="justify"><Para>TMAP_SRP number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>14</Para>
</entry>
<entry colname="2" align="justify"><Para>F051</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than the TMAP_SRP number</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>15</Para>
</entry>
<entry colname="2" align="justify"><Para>F052</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified TMAP_SA is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>16</Para>
</entry>
<entry colname="2" align="justify"><Para>F053</Para>
</entry>
<entry colname="3" align="justify"><Para>MAP_EN number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>17</Para>
</entry>
<entry colname="2" align="justify"><Para>F060</Para>
</entry>
<entry colname="3" align="justify"><Para>C_POSIT exists, but there is no PGMAP in the PGC</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>18</Para>
</entry>
<entry colname="2" align="justify"><Para>F061</Para>
</entry>
<entry colname="3" align="justify"><Para>C_POSIT exists, but the PG number in the PGC is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>19</Para>
</entry>
<entry colname="2" align="justify"><Para>F062</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than the PG number in the PGC</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>20</Para>
</entry>
<entry colname="2" align="justify"><Para>F063</Para>
</entry>
<entry colname="3" align="justify"><Para>C_POSIT exists, but there is no C_PBIT in the PGC</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>21</Para>
</entry>
<entry colname="2" align="justify"><Para>F064</Para>
</entry>
<entry colname="3" align="justify"><Para>C_POSIT exists, but the PG number in the PGC is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>22</Para>
</entry>
<entry colname="2" align="justify"><Para>F065</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified Cell number is 0</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>23</Para>
</entry>
<entry colname="2" align="justify"><Para>F066</Para>
</entry>
<entry colname="3" align="justify"><Para>Specified value is larger than the Cell number in the PGC</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>24</Para>
</entry>
<entry colname="2" align="justify"><Para>F067</Para>
</entry>
<entry colname="3" align="justify"><Para>Must be a block array</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>25</Para>
</entry>
<entry colname="2" align="justify"><Para>F070</Para>
</entry>
<entry colname="3" align="justify"><Para>Is not NV_PCK data</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>26</Para>
</entry>
<entry colname="2" align="justify"><Para>FOB0</Para>
</entry>
<entry colname="3" align="justify"><Para>No Cell number for current search</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>27</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E0</Para>
</entry>
<entry colname="3" align="justify"><Para>No user guide PGC control file for DFD, cannot resolve</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>28</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E1</Para>
</entry>
<entry colname="3" align="justify"><Para>DFD main micro-controller type not compatible, cannot download</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>29</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E2</Para>
</entry>
<entry colname="3" align="justify"><Para>DFD download start; PGC playback error </Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>30</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E3</Para>
</entry>
<entry colname="3" align="justify"><Para>Waiting for DFD download completion; PGC playback error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>31</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E4</Para>
</entry>
<entry colname="3" align="justify"><Para>AVDEC during DFD download</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>32</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E5</Para>
</entry>
<entry colname="3" align="justify"><Para>Firmware file read error during DFD download</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>33</Para>
</entry>
<entry colname="2" align="justify"><Para>F0E6</Para>
</entry>
<entry colname="3" align="justify"><Para>Interpolation check error in read-in DFD firmware</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>34</Para>
</entry>
<entry colname="2" align="justify"><Para>F0F0</Para>
</entry>
<entry colname="3" align="justify"><Para>No firmware file for DFD; download unnecessary</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>35</Para>
</entry>
<entry colname="2" align="justify"><Para>F0F1</Para>
</entry>
<entry colname="3" align="justify"><Para>No firmware matching the DFD download parameters; download unnecessary</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>36</Para>
</entry>
<entry colname="2" align="justify"><Para>F103</Para>
</entry>
<entry colname="3" align="justify"><Para>Illegal Highlight Position</Para>
</entry>
<entry colname="4" align="justify"><Para>Disk &rarr; IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>37</Para>
</entry>
<entry colname="2" align="justify"><Para>F4FF</Para>
</entry>
<entry colname="3" align="justify"><Para>No ACK when requesting forced initialization of panel component</Para>
</entry>
<entry colname="4" align="justify"><Para>Panel Component &rarr; IC6001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>38</Para>
</entry>
<entry colname="2" align="justify"><Para>F500</Para>
</entry>
<entry colname="3" align="justify"><Para>DSC Error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>39</Para>
</entry>
<entry colname="2" align="justify"><Para>F501</Para>
</entry>
<entry colname="3" align="justify"><Para>DSC Not Ready Error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>40</Para>
</entry>
<entry colname="2" align="justify"><Para>F502</Para>
</entry>
<entry colname="3" align="justify"><Para>DSC Time Out Error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>41</Para>
</entry>
<entry colname="2" align="justify"><Para>F503</Para>
</entry>
<entry colname="3" align="justify"><Para>DSC Communication Failure</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>42</Para>
</entry>
<entry colname="2" align="justify"><Para>F504</Para>
</entry>
<entry colname="3" align="justify"><Para>Error adjusting DSC data slice offset</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>43</Para>
</entry>
<entry colname="2" align="justify"><Para>F505</Para>
</entry>
<entry colname="3" align="justify"><Para>DSC Attention Error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>44</Para>
</entry>
<entry colname="2" align="justify"><Para>F506</Para>
</entry>
<entry colname="3" align="justify"><Para>Can&rsquo;t determine media type (invalid media type)</Para>
</entry>
<entry colname="4" align="justify"><Para>IC2001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>45</Para>
</entry>
<entry colname="2" align="justify"><Para>F600</Para>
</entry>
<entry colname="3" align="justify"><Para>Can&rsquo;t access administrative data due to demodulation error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>46</Para>
</entry>
<entry colname="2" align="justify"><Para>F601</Para>
</entry>
<entry colname="3" align="justify"><Para>Undefined sector ID requested</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>47</Para>
</entry>
<entry colname="2" align="justify"><Para>F602</Para>
</entry>
<entry colname="3" align="justify"><Para>Can&rsquo;t&rsquo; access LEAD_IN data due to demodulation error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>48</Para>
</entry>
<entry colname="2" align="justify"><Para>F603</Para>
</entry>
<entry colname="3" align="justify"><Para>Can&rsquo;t access KEY_DET due to demodulation error</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>49</Para>
</entry>
<entry colname="2" align="justify"><Para>F610</Para>
</entry>
<entry colname="3" align="justify"><Para>Can&rsquo;t control ODC</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>50</Para>
</entry>
<entry colname="2" align="justify"><Para>F611</Para>
</entry>
<entry colname="3" align="justify"><Para>No CRCOK within the set time period (CD related)</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>51</Para>
</entry>
<entry colname="2" align="justify"><Para>F612</Para>
</entry>
<entry colname="3" align="justify"><Para>No CRCOK within the set time period (DVD related)</Para>
</entry>
<entry colname="4" align="justify"><Para>IC7001</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>52</Para>
</entry>
<entry colname="2" align="justify"><Para>F620</Para>
</entry>
<entry colname="3" align="justify"><Para>Laser safeguard: high temperature condition</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>53</Para>
</entry>
<entry colname="2" align="justify"><Para>F621</Para>
</entry>
<entry colname="3" align="justify"><Para>Laser safeguard: circuit failure condition</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>54</Para>
</entry>
<entry colname="2" align="justify"><Para>F700</Para>
</entry>
<entry colname="3" align="justify"><Para>MBX Overflow</Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>55</Para>
</entry>
<entry colname="2" align="justify"><Para>F701</Para>
</entry>
<entry colname="3" align="justify"><Para>Message Command Not Complete Error</Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>56</Para>
</entry>
<entry colname="2" align="justify"><Para>F702</Para>
</entry>
<entry colname="3" align="justify"><Para>Message Command Changed</Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>57</Para>
</entry>
<entry colname="2" align="justify"><Para>F880</Para>
</entry>
<entry colname="3" align="justify"><Para>Task number not relevant</Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>58</Para>
</entry>
<entry colname="2" align="justify"><Para>F890</Para>
</entry>
<entry colname="3" align="justify"><Para>Attempted to send message while sending to an AV task (mailbox overflow, etc.)</Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>59</Para>
</entry>
<entry colname="2" align="justify"><Para>F891</Para>
</entry>
<entry colname="3" align="justify"><Para>Couldn&rsquo;t send message to AV task (mailbox overflow, etc.) </Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>60</Para>
</entry>
<entry colname="2" align="justify"><Para>F8A0</Para>
</entry>
<entry colname="3" align="justify"><Para>Message command is not relevant</Para>
</entry>
<entry colname="4" align="justify"><Para>System component bug &rarr; IC6201</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>61</Para>
</entry>
<entry colname="2" align="justify"><Para>F893</Para>
</entry>
<entry colname="3" align="justify"><Para>Flash ROM is interpolated</Para>
</entry>
<entry colname="4" align="justify"><Para>IC6302</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>62</Para>
</entry>
<entry colname="2" align="justify"><Para>F894</Para>
</entry>
<entry colname="3" align="justify"><Para>EEPROM is not normal</Para>
</entry>
<entry colname="4" align="justify"><Para>IC6303</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>63</Para>
</entry>
<entry colname="2" align="justify"><Para>F895</Para>
</entry>
<entry colname="3" align="justify"><Para>Error in language destination (over D6)</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>64</Para>
</entry>
<entry colname="2" align="justify"><Para>F896</Para>
</entry>
<entry colname="3" align="justify"><Para>Setting are for a non-existant model (over D6)</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>65</Para>
</entry>
<entry colname="2" align="justify"><Para>F897</Para>
</entry>
<entry colname="3" align="justify"><Para>Initialization after writing not completing (over D6)</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.575in">
<colspec colnum="2" colname="2" colwidth="1.122in">
<colspec colnum="3" colname="3" colwidth="3.350in">
<colspec colnum="4" colname="4" colwidth="1.856in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>No.</Para>
</entry>
<entry colname="2" align="center"><Para>Error Display</Para>
</entry>
<entry colname="3" align="center"><Para>Error Explanation</Para>
</entry>
<entry colname="4" align="center"><Para>Cause (IC number,etc.)</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>U11</Para>
</entry>
<entry colname="3" align="justify"><Para>Focus servo error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>H01</Para>
</entry>
<entry colname="3" align="justify"><Para>Tray loading error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" morerows="2" align="justify"><Para>3</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="2" morerows="2" align="justify"><Para>H02</Para>
<Para></Para>
<Para></Para>
</entry>
<entry colname="3" align="justify"><Para>Spindle server error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="3" align="justify"><Para>DSC disk motor error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="3" align="justify"><Para>6626 CLVS FAILURE</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>H03</Para>
</entry>
<entry colname="3" align="justify"><Para>Traverse motor error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>H04</Para>
</entry>
<entry colname="3" align="justify"><Para>Tracking server error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>H05</Para>
</entry>
<entry colname="3" align="justify"><Para>SEEK timeout error</Para>
</entry>
<entry colname="4" align="justify"><Para></Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
</item>
</seqlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0901010000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0903000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
