#

9.4.1 Outline

TOP PREVIOUS NEXT

- Since the Mitsubishi M3819 series micro-controller is capable of making programs operate in RAM the pseudo ROM corrections below are possible.

- Program the process calling the modifying sub-routine in advance.

- Program the process to read-out the program from the EEPROM into RAM in advance.

- Processes previous to the read-out cannot be modified.

- In pseudo ROM corrections defective processses cannot be completely bypassed.

TOP PREVIOUS NEXT