#

11.1 Video Output (Brightness Signal) adjustment

TOP PREVIOUS NEXT

Carry out this adjustment after board replacement.

Measurement Point | Adjustment Mode | Test Disc
Video output jac | Colour bar 75%Playback (Title 46) : DVDT-S15Playback (Title 12): DVDT-S15 | DVDT- S15orDVDT-S01
Required equirmentScrewdriver, oscilloscope | Adjustment
1000mVp-p±20mV

Purpose: To ensure compatibility of video signal output.1. Connect the oscilloscope to the video output jacks and set 75Ω.

TOP PREVIOUS NEXT