#

9.3.3 Jitter Offset Correction

TOP PREVIOUS NEXT

- The jitter offset correction function below is necessary for D5, but is not necessary for D8.

- While displaying K objects,certain remote control operations correct the offset of the DVD MODULE jitter value.

- When the DVD module firmware rewriting connector is inserted K objects will be displayed [KC 00 0000].

- Key codes of input from the remote control’s ten key while displaying K objects are relayed to the system component by the operating console.

- Inputting [2] [0] from the remote control returns a 14 hex value from the system component. The value is converted from hex → dec and displayed as [KC 20 0000].

- Continuously pressing the [PLAY] button returns the offset result as a text string from the system component, which is displayed as [KC 20 0002].

- The DVD Module has functions that support buttons other than [2] [0] [PLAY], so when K objects are being displayed key codes are as below.

  [0] [1] [2] [3] [4] [5] [6] [7] [8] [9] [>=10] [PLAY]

TOP PREVIOUS NEXT