#

7.5 Check for Power P.C.B.

TOP PREVIOUS NEXT

- Carry out (Step 1) - (Step 3) in section 7.1

- Carry out (Step 1) - (Step 3) in section 7.4

Step 1 Remove connector at CP705, CN503 and CN501.

Step 6 Connect back connector at CN501 and CN503.

Step 7 Remove wire from connector CN102.

Step 8 Detach FFC at CN1, CP6251, CN1304 and CN806.

- Carry out checks with Power P.C.B. in the condition as indicated in the diagram below.

Step 9 Let the Main P.C.B. stand up.

TOP PREVIOUS NEXT