<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1101000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>11.1 Video Output (Brightness Signal) adjustment</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1100000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1102000000
</nmlist>
</nameloc>
</Para>
<Para>Carry out this adjustment after board replacement.</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="3" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="1.499in">
<colspec colnum="2" colname="2" colwidth="1.769in">
<colspec colnum="3" colname="3" colwidth="3.730in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>Measurement Point</Para>
</entry>
<entry colname="2" align="center"><Para>Adjustment Mode</Para>
</entry>
<entry colname="3" align="center"><Para>Test Disc</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="center"><Para>Video output jac</Para>
</entry>
<entry colname="2" align="center"><Para>Colour bar 75&percnt;Playback (Title 46) : DVDT-S15Playback (Title 12): DVDT-S15</Para>
</entry>
<entry colname="3" align="center"><Para>DVDT- S15orDVDT-S01</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" morerows="1" align="left"><Para>Required equirmentScrewdriver, oscilloscope</Para>
</entry>
<entry namest="2" nameend="3" align="center"><Para>Adjustment</Para>
</entry>
</row>
<row rowsep="0"><entry namest="2" nameend="3" align="center"><Para>1000mVp-p&plusmn;20mV</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>Purpose: To ensure compatibility of video signal output.</Para>
<Para>1. Connect the oscilloscope to the video output jacks and set 75&ohm;.</Para>
<Figure><graphic boardno="graphic105" reprowid="92.626mm" reprodep="59.436mm" location="internal"></Figure>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1100000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1102000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
