#

7.9.1 Disassmbly of Mechanised Drive Part

TOP PREVIOUS NEXT

- Carry out (Step 1) - (Step 3) in section 7.1

- Carry out (Step 1) - (Step 6) in section 7.2

- Carry out (Step 1) - (Step 10) in section 7.7

- Carry out (Step 1) - (Step 8) in section 7.8

Step 2 Remove tab at 1 location and detach the pitch plate.

Step 3 Remove belt and gear changing spring.

Step 4 Remove pulley gear, change gear, UP/DOWN gear.

Step 5 Remove tab at 2 locations and detach the bottom SW board.

Step 6 Temporarily attach the tray lock spring to the catch portion.

Step 7 Remove tab 1 location and detach tray lock.

Step 8 Remove tab 1 location and then remove the rear lock.

Step 9 While pressing tab (B) in direction of arrow (1), press down the connection lever in direction of arrow (2).

Step 10 Move slide plate (R) until the edge of stock side.

Step 11 Lift up the left side of spindle base unit first in direction of arrow (1) and remove in direction of arrow (2).

Step 12 Remove slide plate (R) and slide plate (L).

Step 13 Remove traverse relay gear, traverse cam gear and drive gear.

TOP PREVIOUS NEXT