#

9.4.3 CHECK SUM Display

TOP PREVIOUS NEXT

- In order to confirm that the EEPROM is loaded, the operations below display the CHECK SUMs for the Operating Console, mechanism component, and DSP micro-controller EEPROMs.

- Receiving [1DDF or 1CDF] when in Process Check Mode with Process Check Mode-in [1DDF or 1 CDF] will display the operating console’s version and EEPROM CHECK SUM.

- If [1DDF or 1CDF] are received while the operating console’s version and EEPROM CHECK SUM are being displayed the mechanism component’s version and EEPROM CHECK SUM are displayed.

- If [1DDF or 1CDF] are received while the mechanism component’s version and EEPROM CHECK SUM are being displayed the DSP micro-controller’s version and EEPROM CHECK SUM are displayed.

- If a valid remote control code is received while the CHECK SUM is being displayed the CHECK SUM display will be erased to confirm with that operation and display.

- When the result of referencing the EEPROM is a differing file name [NO] will be displayed, just as when no EEPROM is present.

TOP PREVIOUS NEXT