#

7.9.2 Disassembly and assembly of Spindle Base Unit

TOP PREVIOUS NEXT

Step 1 Pull out 5 numbers of disc spacers after pressing down the bottom hook with a fine-tip minus screwdriver.

Step 2 While pressing the tab, slide the support plate in direction of arrow and remove the support plate.

Step 3 Pull out the disc lever with the disc lever turned in the direction of arrow (1).

Step 4 Remove tab at 2 locations and pull out relay gear (B).

Step 5 Remove tab at 2 locations.

Step 6 Remove cushion spring.

Step 7 Remove rotation stopper (semi) in direction of arrow.

Step 8 Remove tab at 2 locations and pull out relay gear (A).

Step 9 Remove tab at 2 locations and detach the spindle shaft.

Step 10 Remove bottom spindle spring with a pair of tweezer.

Step 11 Press down the bottom hook with a fine-tip minus screwdriver.

Step 12 Hold the axis part of the bottom hook and pull it out.

Step 13 Turn the bottom spindle in the direction of arrow until it hits against the stopper.

Step 14 Insert a fine-tip minus screwdriver between the bottom spindle and UP/DOWN base and slightly raise the bottom spindle for it to go over the stopper. Then turn the bottom spindle and remove it.

Step 15 Rotate the UP/DOWN base 90°. The spread the leg portion of the rotation stopper and remove the UP/DOWN base.

TOP PREVIOUS NEXT