#

1 Safety Precaution

TOP PREVIOUS NEXT

(This “Safety Precaution” is applied only in U.S.A.)

1. Before servicing, unplug the power cord to prevent an electric shock.

2. When replacing parts, use only manufacturer’s recommended components for safety.

3. Check the condition of the power cord. Replace if wear or damage is evident.

4. After servicing, be sure to restore the lead dress, insulation barriers, insulation papers, shields, etc.

5. Before returning the serviced equipment to the customer, be sure to make the following insulation resistance test to

   prevent the customer from being exposed to a shock hazard.

1.1 Insulation Resistance Test

TOP PREVIOUS NEXT