#

9.4.2 EERPOM Flag Indicator Interpretation

TOP PREVIOUS NEXT

- Regardless of the EEPROM flag indicator CS/CLK/DATA is output and the DATA read-in process occurs.

  Accordingly, even if there is no EEPROM hardware processing at the terminal is necessary.

- If the data read-out below is valid then an EEPROM will be determined to be present, and the modifying program will be read-out.

  - When the MASK ROM file name (8 character ASCII code, 8 bytes) and the EEPROM file name match.

  - When the modifying points flag indicator data (8 points, 1 byte) written at two places on the EEPROM match.

TOP PREVIOUS NEXT