<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT67P</Model>
<System>ORDER NO. MD0203047C1</System>
<SubSystem>DVD Home Theatre Sound System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0709010000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=Jan year=2003>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT67P</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>7.9.1 Disassmbly of Mechanised Drive Part</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0709000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0709020000
</nmlist>
</nameloc>
</Para>
<Para><randlist prefix=unorder><item><Para>Carry out (Step 1) - (Step 3) in section 7.1</Para>
</item>
<item><Para>Carry out (Step 1) - (Step 6) in section 7.2</Para>
</item>
<item><Para>Carry out (Step 1) - (Step 10) in section 7.7</Para>
</item>
<item><Para>Carry out (Step 1) - (Step 8) in section 7.8</Para>
</item>
</randlist>
</Para>
<Figure><graphic boardno="graphic51" reprowid="74.613mm" reprodep="66.146mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
 Remove tab at 1 location and detach the pitch plate.</Para>
<Figure><graphic boardno="graphic52" reprowid="77.259mm" reprodep="67.028mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
 Remove belt and gear changing spring.</Para>
<Figure><graphic boardno="graphic53" reprowid="70.379mm" reprodep="64.735mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
 Remove pulley gear, change gear, UP&sol;DOWN gear.</Para>
<Para></Para>
<Para></Para>
<Para><emphasis>Step 5</emphasis>
 Remove tab at 2 locations and detach the bottom SW board.</Para>
<Figure><graphic boardno="graphic54" reprowid="91.193mm" reprodep="155.223mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
 Temporarily attach the tray lock spring to the catch portion.</Para>
<Para><emphasis>Step 7</emphasis>
 Remove tab 1 location and detach tray lock.</Para>
<Figure><graphic boardno="graphic55" reprowid="83.961mm" reprodep="106.186mm" location="internal"></Figure>
<Para><emphasis>Step 8</emphasis>
 Remove tab 1 location and then remove the rear lock.</Para>
<Figure><graphic boardno="graphic56" reprowid="85.902mm" reprodep="107.950mm" location="internal"></Figure>
<Para><emphasis>Step 9</emphasis>
 While pressing tab (B) in direction of arrow (1), press down the connection lever in direction of arrow (2).</Para>
<Figure><graphic boardno="graphic57" reprowid="62.618mm" reprodep="72.672mm" location="internal"></Figure>
<Para><emphasis>Step 10</emphasis>
 Move slide plate (R) until the edge of stock side.</Para>
<Figure><graphic boardno="graphic58" reprowid="82.021mm" reprodep="64.735mm" location="internal"></Figure>
<Para><emphasis>Step 11</emphasis>
 Lift up the left side of spindle base unit first in direction of arrow (1) and remove in direction of arrow (2).</Para>
<Figure><graphic boardno="graphic59" reprowid="81.492mm" reprodep="85.725mm" location="internal"></Figure>
<Figure><graphic boardno="graphic60" reprowid="86.078mm" reprodep="77.788mm" location="internal"></Figure>
<Para><emphasis>Step 12</emphasis>
 Remove slide plate (R) and slide plate (L).</Para>
<Figure><graphic boardno="graphic61" reprowid="80.963mm" reprodep="61.736mm" location="internal"></Figure>
<Para><emphasis>Step 13</emphasis>
 Remove traverse relay gear, traverse cam gear and drive gear.</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
svcml
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0709000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0709020000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
