#

7.7 Replacement of DVD Traverse Unit

TOP PREVIOUS NEXT

- Carry out (Step 1) - (Step 3) in section 7.1

- Carry out (Step 1) - (Step 6) in section 7.2

Step 1 Pull out the FFC at 3 locations.

Step 2 Detach the connector.

Step 3 Detach the DVD loading unit.

Step 4 Remove the top plate.

Step 5 Insert the hexagon driver (gear) into the hole.

Step 6 Turn the hexagon driver clockwise to fully open the disc tray.

Step 7 When tab (B) is pressed in direction of arrow(1), the connection lever moves in the direction of arrow (2).

Step 8 Turn the hexagon driver clockwise with tab (A) in depressed condition.

Step 10 Let the Main P.C.B. stand up.

TOP PREVIOUS NEXT