#

7.9.3 Installation of Rotation Stopper (Semi)

TOP PREVIOUS NEXT

Step 1 Fit the tab on rotation stopper (semi) into the opening on spindle base. (Be careful as the size of tab differs).

Step 2 Lower down the rotation stopper (semi) and fit the trapezoidal tooth between bottom spindle and relay gear A.

Step 3 Insert the rotation stopper (semi) and ensure that the tabs are engaged.

TOP PREVIOUS NEXT