<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0804000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>8.4 Disassembly and assembly of the Disc Tray</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0803000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0900000000x
</nmlist>
</nameloc>
</Para>
<Figure><graphic boardno="graphic31" reprowid="75.904mm" reprodep="77.513mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
With lifting the claw in the direction of arrow 1, draw the clamp SW P.C.B. in the direction of arrow 2.</Para>
<Para><emphasis>Step 3</emphasis>
Remove the mechanism cover.</Para>
<Figure><graphic boardno="graphic32" reprowid="79.248mm" reprodep="72.983mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
Insert the gear with hexagonal wrench into the hole.</Para>
<Figure><graphic boardno="graphic33" reprowid="79.248mm" reprodep="61.510mm" location="internal"></Figure>
<Para><emphasis>Step 5</emphasis>
Rotate the hexagonal wrench in the direction of arrow (clockwise), and then open the disc tray fully.</Para>
<Figure><graphic boardno="graphic34" reprowid="88.000mm" reprodep="86.233mm" location="internal"></Figure>
<Para><emphasis>Step 6</emphasis>
Upset the CD changer unit again.</Para>
<Para><emphasis>Step 7</emphasis>
Release both the claws, and then draw the disc tray.</Para>
<Figure><graphic boardno="graphic35" reprowid="83.693mm" reprodep="90.763mm" location="internal"></Figure>
<Para><emphasis>Step 8</emphasis>
With forcing the left guide bar manually because the left guide bar interfers with claw, draw the disc tray.</Para>
<Para><randlist prefix=unorder><item><Para><emphasis>Installation of the disc tray after replacement</emphasis>
</Para>
<Figure><graphic boardno="graphic36" reprowid="75.692mm" reprodep="52.282mm" location="internal"></Figure>
</item>
</randlist>
</Para>
<Para><emphasis>Step 1</emphasis>
Slide the drive rack fully in the direction of arrow.</Para>
<Figure><graphic boardno="graphic37" reprowid="55.330mm" reprodep="80.688mm" location="internal"></Figure>
<Para><emphasis>Step 2</emphasis>
Holding the drive rack not to move, install the disc tray.</Para>
<Figure><graphic boardno="graphic38" reprowid="73.745mm" reprodep="84.667mm" location="internal"></Figure>
<Para><emphasis>Step 3</emphasis>
Align the drive rack with the driver gear.</Para>
<Figure><graphic boardno="graphic39" reprowid="79.248mm" reprodep="62.696mm" location="internal"></Figure>
<Para><emphasis>Step 4</emphasis>
Holding the disc tray manually, rotate the pulley gear in the direction of arrow.</Para>
<Para><emphasis>Step 5</emphasis>
Rotate the gear 5 or 6 times manually, and then push the disc tray.</Para>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0803000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0900000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
