<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1002000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title>10.2 Error detection for CD&sol;Changer block</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1001000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1003000000
</nmlist>
</nameloc>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.630in"><colspec colnum="2" colname="2" colwidth="1.936in"><colspec colnum="3" colname="3" colwidth="0.707in"><colspec colnum="4" colname="4" colwidth="3.698in"><thead><row rowsep="1"><entry colname="1" align="center"><Para>No.</Para>
</entry>
<entry colname="2" align="left"><Para>Error</Para>
</entry>
<entry colname="3" align="center">Error<Para>Display</Para>
</entry>
<entry colname="4" align="left"><Para>Problem condition</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="center"><Para>1</Para>
</entry>
<entry colname="2" align="left"><Para>REST SW detection error</Para>
</entry>
<entry colname="3" align="center"><Para>F15</Para>
</entry>
<entry colname="4" align="left">CD does not function.<Para>This error occurs when the Optical Pick Up REST SW (S701) is not</Para>
<Para>detected within the specified time (about 8 seconds)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>2</Para>
</entry>
<entry colname="2" align="left"><Para>CD tray opens automatically</Para>
</entry>
<entry colname="3" align="center"><Para>F16</Para>
</entry>
<entry colname="4" align="left"><Para>CLAMP switch (S4) NG (Check &amp; Replace)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>3</Para>
</entry>
<entry colname="2" align="left">Does not startup when [PLAY]<Para>button is pressed</Para>
</entry>
<entry colname="3" align="center"><Para>F17</Para>
</entry>
<entry colname="4" align="left"><Para>BOTTOM switch (S5) NG (Check &amp; Replace)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>4</Para>
</entry>
<entry colname="2" align="left">Transmission error between CD<Para>servo LSI and micon</Para>
</entry>
<entry colname="3" align="center"><Para>F26</Para>
</entry>
<entry colname="4" align="left">CD does not function.<Para>This error occurs when the POWER is ON for the CD block and an error is</Para>
<Para>detected after the transmission has started.</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>5</Para>
</entry>
<entry colname="2" align="left">Startup fails even when you<Para>insert CD or the selected disc tray</Para>
<Para>does not open</Para>
</entry>
<entry colname="3" align="center"><Para>F27</Para>
</entry>
<entry colname="4" align="left"><Para>Tray 1 detect switch or Tray 2 detect switch NG (Check &amp; Replace)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>6</Para>
</entry>
<entry colname="2" align="left"><Para>Cannot insert CD</Para>
</entry>
<entry colname="3" align="center"><Para>F28</Para>
</entry>
<entry colname="4" align="left"><Para>Tray 1 detect switch NG (Check &amp; Replace)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="center"><Para>7</Para>
</entry>
<entry colname="2" align="left"><Para>Cannot eject CD</Para>
</entry>
<entry colname="3" align="center"><Para>F29</Para>
</entry>
<entry colname="4" align="left"><Para>Check if disc is stuck. Tray 2 detect switch NG (Confirm &amp; Replace)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="center"><Para>8</Para>
</entry>
<entry colname="2" align="left"><Para>The CD tray closes</Para>
</entry>
<entry colname="3" align="center"><Para>H15</Para>
</entry>
<entry colname="4" align="left"><Para>CD disc tray detect switch NG (S3) (Check &amp; Replace)</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para></Para>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1001000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1003000000
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
