<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >
<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >
<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-PM11</Model>
<System>ORDER NO. MD0102023C1</System>
<SubSystem>CD Stereo System</SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0000000000</ModuleTitle>
<IssueNo issue=3>
<IssueDate day=10 month=May year=2001>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-PM11</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>
<Body>
<Descriptive>
<Title id=cover>Service Manual</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0100000000x
</nmlist>
</nameloc>
</Para>
<Para>ORDER NO. MD0102023C1</Para>
<Para>A6</Para>
<Figure><graphic boardno="mttl1" location="internal"></Figure>
<Status><Subsystem>CD Stereo System</Subsystem>
<Figure><graphic boardno="logo1" location="internal"></Figure>
<Para><randlist prefix=simple><item><Para>SA-PM11</Para>
</item>
</randlist>
</Para>
<Para></Para>
<Para>Colour</Para>
<Para>(S)... Silver Type</Para>
<Para>(A)... Blue Type</Para>
<Para></Para>
<Para>Area</Para>
<Para>(P)... U.S.A.</Para>
<Para>(PC)... Canada</Para>
<Para></Para>
<Para>TAPE SECTION :</Para>
<Para>AR2 MECHANISM SERIES</Para>
<Para>CD SECTION :</Para>
<Para>RAE0152Z-3 TRAVERSE DECK SERIES</Para>
</Status>
<Figure><graphic boardno="mdlpic2" reprowid="84.159MM" reprodep="51.139MM" location="internal"></Figure>
<Table frame="NONE" colsep="0" rowsep="0"><Title> Specifications</Title>
<tgroup cols="2" colsep="0" rowsep="0"><colspec colnum="1" colname="1" colwidth="1.742in" colsep="0"><colspec colnum="2" colname="2" colwidth="1.742in" colsep="0"><tbody><row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; AMPLIFIER SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Power output</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>10&percnt; Total harmonic distortion</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>1 kHz, both channels driven</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>45 W per channel (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="JUSTIFY"><Para>70 Hz - 16 kHz, both channels driven</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>40 W per channel (6&ohm;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Input sensitivity</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>AUX</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>250 mV</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Input Impedance</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>AUX</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>13 k&ohm; </Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; FM TUNER SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Frequency range</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>87.9 - 107.9 MHz (200 kHz steps)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>87.5 - 108.0 MHz (100 kHz steps)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Sensitivity</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>2.5&micro;V (IHF)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>S&sol;N 26 dB</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>2.2&micro;V</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Antenna terminal(s)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>75&ohm; (unbalanced)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; AM TUNER SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Frequency range</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>AM</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>520-1710 kHz MHz (10 kHz steps)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Sensitivity</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>AM</Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>S&sol;N 20 dB (at 1000kHz)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>560&micro;V&sol;m</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Antenna terminal(s)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>75&ohm; (unbalanced)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; CASSETTE DECK SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Track system</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>4 track, 2 channel</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Heads</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Record&sol;playback</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Solid permalloy head</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Erasure</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Double gap ferrite head</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Motor</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>DC servo motor</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Recording system</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>AC bias 100 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Erasing system</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>AC erase 100 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Tape speed</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>4.8 cm&sol;s</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="LEFT"><Para>Frequency response (&plus;3 dB, -6 dB at DECK OUT)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="LEFT"><Para>NORMAL (TYPE I)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>50 Hz - 13 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>HIGH (TYPE II)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>50 Hz - 13 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>S&sol;N</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>50 dB (A weighted)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Wow and flutter</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>0.18&percnt; (WRMS)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Fast forward and rewind time</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Approx. 120 seconds with</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>C-60 cassette tape</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; CD SECTION</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Sampling frequency</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>44.1 kHz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Decoding</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>16 bit linear</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Beam source&sol;wave length</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Semiconductor laser&sol;780 nm</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Number of channels</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Stereo</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Frequency response</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>20 Hz - 20 kHz (&plus;1, -2 dB)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Wow and flutter</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Below measurable limit</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Digital filter</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>8 fs</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>D&sol;A converter</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>MASH (1 bit DAC)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; GENERAL</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Power supply</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>AC 120 V, 60Hz</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Power consumption</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>125 W</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Dimensions (W x H x D)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>200 x 260 x 345 mm</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>(5 29&sol;32&rdquo; x 10 1&sol;4&rdquo; x 10 1&sol;2&rdquo;)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>Weight</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>5.6 kg (12.3 lb)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="JUSTIFY"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para><emphasis>&block; SYSTEM</emphasis>
</Para>
</entry>
<entry colname="2" align="RIGHT"><Para></Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>SC-PM11(P)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Music Center: SA-PM11(P)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Speaker: SB-PM11(P)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para>SC-PM11(PC)</Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Music Center: SA-PM11(PC)</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="JUSTIFY"><Para></Para>
</entry>
<entry colname="2" align="RIGHT"><Para>Speaker: SB-PM11(P)</Para>
</entry>
</row>
<row rowsep="0"><entry namest="1" nameend="2" align="LEFT"><Para><emphasis>Notes:</emphasis>
</Para>
<Para><seqlist><item><Para>Specifications are subject to change without notice. Weight and dimensions are aproximate.</Para>
</item>
<item><Para>Total harmonic distortion is measured by the digital spectrum analyzer.</Para>
</item>
</seqlist>
</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>
<Para>&copy; 2001 Matsushita Electronics (S) Pte. Ltd. All rights reserved. Unauthorized copying and distribution is a violation of law.</Para>
<SafetyPara><Warning><Para><graphic boardno="graphic1" reprowid="183.000MM" reprodep="21.406MM" location="internal"></Para>
</Warning>
</SafetyPara>
<Figure><graphic boardno="bnm2" location="internal"></Figure>
<!-- Footer -->
<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
sapm11pp
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0100000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>
&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
